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Sartorius Stedim Biotech FuB filter housings were developed for sanitary beverage filtration applications, including:

· Beer
· Wine u spirits
· Mineral | Bottled water
· Carbonated Soft drinks
· Non-carbonated Soft drinks

Thanks to their optimized design, our FuB housings are exceptionally easy to clean for thorough results and can be in-line steam sterilized as a complete unit, incl. gaskets.

Our housings have been designed in accordance with the European Pressure Equipment Directive PED 2014/68/EU - rule EN13445.

The complete series of 810 and 813 housings are available in sizes ranging from 1 to 30 cartridges and heights from 10“ to 40“.

The cartridge socket adapter is available in code 25 (code 7) and code 28 (810 liquid u 813 liquid).

Sartorius Stedim Biotech FuB housings can be equipped with
a wide range of Inlet and Outlet connections such as DIN11851 and sanitary Clamp. Other connections are available upon request. Vent and drain options are also available in multiple designs and configurations.

Gaskets are offered in various material types depending on
the application. As standard, we use FDA, USP Class VI, EC 1935/2004 arti- cle 3 - u Phthalate-free compliant Silicone u EPDM
elastomers.

Certification is according to PED 2014/68/EU. Additional certificates like Ra roughness or material certificates (MTR‘s) are available upon request.

Only 316L grade stainless steel is used for all wetted surfaces to provide maximum durability and resistance to corrosion.
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*Gas Housings 10 bar only available in 1-round
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Working pressure:	max.13 bar | 189 psi Temperature:	 max. 40°C | 104°F

Working pressure:	 max.4 bar | 58 psi Temperature:	max. 150°C | 302°F

Cartridge adapter	25 | Code 7
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	R mm
	S mm
	N mm
	C mm
	E mm
	VOLUME liters (V)
	PED Category

	01 x 10“
	360
	312
	208
	790
	300
	3.0
	4.3

	01 x 20“
	360
	312
	208
	1040
	550
	4.8
	4.3

	01 x 30“
	360
	312
	208
	1290
	800
	6.8
	I

	01 x 40“
	360
	312
	208
	1540
	1050
	8.6
	I



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	1.0“ (25.4mm x 1.65mm)
	381
	188
	103
	381
	269
	154



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	DN25
	381
	220
	118
	381
	300
	169



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.0“ (25.4mm x 1.65mm)
	381
	163
	90
	381
	244
	141



	PACKAGING SIZE AND WEIGHT

	CARTRIDGE x HEIGHT (N)
	BOWL WEIGHT [kg]
	TOTAL NET WEIGHT [kg]
	PACKAGING SIZE [cm]
	TOTAL WEIGHT PACKED [kg]

	01 x 10“
	2.0
	7.0
	65x27x17
	8.0

	01 x 20“
	3.3
	8.2
	87x27x17
	9.5

	01 x 30“
	4.6
	9.4
	112x27x17
	11.0

	01 x 40“
	5.9
	10.6
	137x27x17
	13.0


FILTER SERIES 810 - 01-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
Page 2 | 4
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.0“

	
	01
	10“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	x

	
	01
	10“
	DIN 11851 Male Part
	DN 25
	EPDM
	x
	x

	
	01
	10“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	-

	
	01
	10“
	DIN 11851 Male Part
	DN 25
	EPDM
	X
	-

	
	01
	10“
	TC
	1“
	Silicone
	x
	x

	
	01
	10“
	TC
	1“
	EPDM
	x
	x

	
	01
	10“
	TC
	1“
	Silicone
	x
	-

	
	01
	10“
	TC
	1“
	EPDM
	x
	-

	
	01
	10“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	x

	
	01
	10“
	Welding Stubs
	25.4 x 1.65
	EPDM
	x
	x

	
	01
	10“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	-

	
	01
	10“
	Welding Stubs
	25.4 x 1.65
	EPDM
	x
	-

	
	01
	20“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	x

	
	01
	20“
	DIN 11851 Male Part
	DN 25
	EPDM
	x
	x

	
	01
	20“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	-

	
	01
	20“
	DIN 11851 Male Part
	DN 25
	EPDM
	x
	-

	
	01
	20“
	TC
	1“
	Silicone
	x
	x

	
	01
	20“
	TC
	1“
	EPDM
	x
	x

	
	01
	20“
	TC
	1“
	Silicone
	x
	-

	
	01
	20“
	TC
	1“
	EPDM
	x
	-

	
	01
	20“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	x

	
	01
	20“
	Welding Stubs
	25.4 x 1.65
	EPDM
	x
	x

	
	01
	20“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	-

	
	01
	20“
	Welding Stubs
	25.4 x 1.65
	EPDM
	x
	-

	
	01
	30“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	x

	
	01
	30“
	DIN 11851 Male Part
	DN 25
	EPDM
	x
	x

	
	01
	30“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	-

	
	01
	30“
	DIN 11851 Male Part
	DN 25
	EPDM
	x
	-

	
	01
	30“
	TC
	1“
	Silicone
	x
	x

	
	01
	30“
	TC
	1“
	EPDM
	x
	x

	
	01
	30“
	TC
	1“
	Silicone
	x
	-

	
	01
	30“
	TC
	1“
	EPDM
	x
	-

	
	01
	30“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	x

	
	01
	30“
	Welding Stubs
	25.4 x 1.65
	EPDM
	x
	x

	
	01
	30“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	-

	
	01
	30“
	Welding Stubs
	25.4 x 1.65
	EPDM
	x
	-

	
	01
	40“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	x

	
	01
	40“
	DIN 11851 Male Part
	DN 25
	EPDM
	x
	x

	
	01
	40“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	-

	
	01
	40“
	DIN 11851 Male Part
	DN 25
	EPDM
	x
	-

	
	01
	40“
	TC
	1“
	Silicone
	x
	x

	
	01
	40“
	TC
	1“
	EPDM
	x
	x

	
	01
	40“
	TC
	1“
	Silicone
	x
	-

	
	01
	40“
	TC
	1“
	EPDM
	x
	-

	
	01
	40“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	x

	
	01
	40“
	Welding Stubs
	25.4 x 1.65
	EPDM
	x
	x

	
	01
	40“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	-

	
	01
	40“
	Welding Stubs
	25.4 x 1.65
	EPDM
	x
	-


XX = 25 (Adapter 25 / code 7)	8
XX = 28 (Sartorius Adapter 28 tripple Bayonet)
FILTER SERIES 810 - 01-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
Page 3 | 4









	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	CLAMP 4“
	AISI 304
	
	1

	3a
	CLAMP
	AISI 316L
	
	1

	3
	CARFTRIDGES PLATE + BENDS
	AISI 316L
	
	1

	
4
	GASKET CLAMP 4“
	SILICONE
	
	1

	
	GASKET CLAMP 4“
	EPDM
	
	1

	5
	LEG
	AISI 304
	
	3


[image: ]
FILTER SERIES 810 - 01-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
Page 4 | 4
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[image: ]Fluid group 1 (dangerous) on request
article no., price u delivery time can be different.
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	R mm
	S mm
	N mm
	C mm
	E mm
	VOLUME liters (V)
	PED Category

	03 x 10“
	357
	310
	206
	816
	290
	7.3
	I

	03 x 20“
	357
	310
	206
	1065
	540
	12.6
	I

	03 x 30“
	357
	310
	206
	1314
	790
	17.8
	I

	03 x 40“
	357
	310
	206
	1564
	1040
	23.1
	II



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	1.5“ (38.1mm x 1.65mm)
	345
	310
	147
	345
	385
	223



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	DN40
	345
	351
	168
	345
	426
	243



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.5“ (38.1mm x 1.65mm)
	345
	285
	135
	345
	360
	210



	PACKAGING SIZE AND WEIGHT

	CARTRIDGE x HEIGHT (N)
	BOWL WEIGHT [kg]
	TOTAL NET WEIGHT [kg]
	PACKAGING SIZE [cm]
	TOTAL WEIGHT PACKED [kg]

	03 x 10“
	4.0
	17.4
	80x30x37
	23.0

	03 x 20“
	6.0
	19.4
	104x30x37
	25.0

	03 x 30“
	8.0
	21.4
	130x30x37
	27.0

	03 x 40“
	10.0
	23.4
	155x30x37
	29.0




Please Note
In filter housings with a flange connection at the in- and outlet e.g. DIN-EN1092-1, ANSI, etc. the bends will be welded directly to the baseplate, instead of the standard flange connection described in the detailed drawing.
FILTER SERIES 810 - 03-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
Page 2 | 4
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	03
	20“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	x

	
	03
	20“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	x

	
	03
	20“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	-

	
	03
	20“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	-

	
	03
	20“
	TC
	1.5“
	Silicone
	x
	x

	
	03
	20“
	TC
	1.5“
	EPDM
	x
	x

	
	03
	20“
	TC
	1.5“
	Silicone
	x
	-

	
	03
	20“
	TC
	1.5“
	EPDM
	x
	-

	
	03
	20“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	x

	
	03
	20“
	Welding Stubs
	38.1 x 1.65
	EPDM
	x
	x

	
	03
	20“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	-

	
	03
	20“
	Welding Stubs
	38.1 x 1.65
	EPDM
	x
	-

	
	03
	30“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	x

	
	03
	30“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	x

	
	03
	30“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	-

	
	03
	30“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	-

	
	03
	30“
	TC
	1.5“
	Silicone
	x
	x

	
	03
	30“
	TC
	1.5“
	EPDM
	x
	x

	
	03
	30“
	TC
	1.5“
	Silicone
	x
	-

	
	03
	30“
	TC
	1.5“
	EPDM
	x
	-

	
	03
	30“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	x

	
	03
	30“
	Welding Stubs
	38.1 x 1.65
	EPDM
	x
	x

	
	03
	30“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	-

	
	03
	30“
	Welding Stubs
	38.1 x 1.65
	EPDM
	x
	-

	
	03
	40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	x

	
	03
	40“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	x

	
	03
	40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	-

	
	03
	40“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	-

	
	03
	40“
	TC
	1.5“
	Silicone
	x
	x

	
	03
	40“
	TC
	1.5“
	EPDM
	x
	x

	
	03
	40“
	TC
	1.5“
	Silicone
	x
	-

	
	03
	40“
	TC
	1.5“
	EPDM
	x
	-

	
	03
	40“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	x

	
	03
	40“
	Welding Stubs
	38.1 x 1.65
	EPDM
	x
	x

	
	03
	40“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	-

	
	03
	40“
	Welding Stubs
	38.1 x 1.65
	EPDM
	x
	-













XX = 25 (Adapter 25 / code 7)	12
XX = 28 (Sartorius Adapter 28 tripple Bayonet)
FILTER SERIES 810 - 03-ROUND LIQUID HOUSING
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	V-BAND
	AISI 304
	
	1

	3
	CARTRIDGE PLATE
	AISI 316L
	
	1

	4
	O-RING d=5.35 ID=158.11
	SILICONE
	
	1

	5
	GASKET CLAMP 1.5“
	PTFE
	
	2

	6
	BEND FLANGE
	AISI 304
	
	4

	7
	INLET BEND
	AISI 316L
	
	1

	8
	OUTLET BEND
	AISI 316L
	
	1

	9
	COMPLETE LEG
	AISI 304
	
	3

	11
	PROTECTION PLATE
	AISI 316L
	
	1






[image: ]
FILTER SERIES 810 - 03-ROUND LIQUID HOUSING
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[image: ]Fluid group 1 (dangerous) on request
article no., price u delivery time can be different.
FILTER SERIES 810 - 05-ROUND LIQUID HOUSING
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	R mm
	S mm
	N mm
	C mm
	E mm
	VOLUME liters (V)
	PED Category

	05 x 10“
	400
	347
	231
	825
	290
	11
	I

	05 x 20“
	400
	347
	231
	1075
	540
	20
	II

	05 x 30“
	400
	347
	231
	1325
	790
	29.1
	II

	05 x 40“
	400
	347
	231
	1575
	1040
	38.2
	II



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	2.0“ (50.8mm x 1.65mm)
	315
	378
	196
	315
	445
	263



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	DN50
	315
	423
	218
	315
	490
	285



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.0“ (50.8mm x 1.65mm)
	315
	353
	183
	315
	420
	250



	PACKAGING SIZE AND WEIGHT

	CARTRIDGE x HEIGHT (N)
	BOWL WEIGHT [kg]
	TOTAL NET WEIGHT [kg]
	PACKAGING SIZE [cm]
	TOTAL WEIGHT PACKED [kg]

	05 x 10“
	5.3
	11.0
	72x35x37
	24.0

	05 x 20“
	7.5
	20.0
	97x35x37
	26.0

	05 x 30“
	10.2
	22.0
	122x35x37
	28.0

	05 x 40“
	12.9
	24.0
	147x35x37
	30.0




Please Note
In filter housings with a flange connection at the in- and outlet e.g. DIN-EN1092-1, ANSI, etc. the bends will be welded directly to the baseplate, instead of the standard flange connection described in the detailed drawing.
FILTER SERIES 810 - 05-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
Page 2 | 4
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	05
	20“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	x

	
	05
	20“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	x

	
	05
	20“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	-

	
	05
	20“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	-

	
	05
	20“
	TC
	2“
	Silicone
	x
	x

	
	05
	20“
	TC
	2“
	EPDM
	x
	x

	
	05
	20“
	TC
	2“
	Silicone
	x
	-

	
	05
	20“
	TC
	2“
	EPDM
	x
	-

	
	05
	20“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	x

	
	05
	20“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	x

	
	05
	20“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	-

	
	05
	20“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	-

	
	05
	30“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	x

	
	05
	30“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	x

	
	05
	30“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	-

	
	05
	30“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	-

	
	05
	30“
	TC
	2“
	Silicone
	x
	x

	
	05
	30“
	TC
	2“
	EPDM
	x
	x

	
	05
	30“
	TC
	2“
	Silicone
	x
	-

	
	05
	30“
	TC
	2“
	EPDM
	x
	-

	
	05
	30“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	x

	
	05
	30“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	x

	
	05
	30“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	-

	
	05
	30“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	-

	
	05
	40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	x

	
	05
	40“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	x

	
	05
	40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	-

	
	05
	40“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	-

	
	05
	40“
	TC
	2“
	Silicone
	x
	x

	
	05
	40“
	TC
	2“
	EPDM
	x
	x

	
	05
	40“
	TC
	2“
	Silicone
	x
	-

	
	05
	40“
	TC
	2“
	EPDM
	x
	-

	
	05
	40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	x

	
	05
	40“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	x

	
	05
	40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	-

	
	05
	40“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	-













XX = 25 (Adapter 25 / code 7)	16
XX = 28 (Sartorius Adapter 28 tripple Bayonet)
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	V-BAND
	AISI 304
	
	1

	3
	CARTRIDGE PLATE
	AISI 316L
	
	1

	4
	O-RING d=5.35 ID=208.91
	SILICONE
	
	1

	5
	GASKET CLAMP 2“
	PTFE
	
	2

	6
	BEND FLANGE
	AISI 304
	
	4

	7
	INLET BEND
	AISI 316L
	
	1

	8
	OUTLET BEND
	AISI 316L
	
	1

	9
	COMPLETE LEG
	AISI 304
	
	3

	11
	PROTECTION PLATE
	AISI 316L
	
	1





[image: ]
FILTER SERIES 810 - 05-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
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[image: ]Fluid group 1 (dangerous) on request
article no., price u delivery time can be different.
FILTER SERIES 810 - 08-ROUND LIQUID HOUSING
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	R mm
	S mm
	N mm
	C mm
	E mm
	VOLUME liters (V)
	PED Category

	08 x 10“
	448
	388
	259
	846
	290
	21.3
	II

	08 x 20“
	448
	388
	259
	1096
	540
	35.5
	II

	08 x 30“
	448
	388
	259
	1346
	790
	48.7
	II

	08 x 40“
	448
	388
	259
	1596
	1040
	63.9
	II



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	2.0“ (50.8mm x 1.65mm)
	315
	404
	222
	315
	471
	289



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	DN50
	315
	449
	244
	315
	516
	311



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.0“ (50.8mm x 1.65mm)
	315
	379
	209
	315
	446
	273



	PACKAGING SIZE AND WEIGHT

	CARTRIDGE x HEIGHT (N)
	BOWL WEIGHT [kg]
	TOTAL NET WEIGHT [kg]
	PACKAGING SIZE [cm]
	TOTAL WEIGHT PACKED [kg]

	08 x 10“
	7.0
	27.0
	75x40x42
	30.0

	08 x 20“
	10.0
	30.0
	100x40x42
	34.0

	08 x 30“
	13.0
	3.0
	125x40x42
	38.0

	08 x 40“
	16.0
	36.0
	150x40x42
	42.0




Please Note
In filter housings with a flange connection at the in- and outlet e.g. DIN-EN1092-1, ANSI, etc. the bends will be welded directly to the baseplate, instead of the standard flange connection described in the detailed drawing.
FILTER SERIES 810 - 08-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
Page 2 | 4
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	08
	20“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	x

	
	08
	20“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	x

	
	08
	20“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	-

	
	08
	20“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	-

	
	08
	20“
	TC
	2“
	Silicone
	x
	x

	
	08
	20“
	TC
	2“
	EPDM
	x
	x

	
	08
	20“
	TC
	2“
	Silicone
	x
	-

	
	08
	20“
	TC
	2“
	EPDM
	x
	-

	
	08
	20“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	x

	
	08
	20“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	x

	
	08
	20“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	-

	
	08
	20“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	-

	
	08
	30“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	x

	
	08
	30“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	x

	
	08
	30“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	-

	
	08
	30“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	-

	
	08
	30“
	TC
	2“
	Silicone
	x
	x

	
	08
	30“
	TC
	2“
	EPDM
	x
	x

	
	08
	30“
	TC
	2“
	Silicone
	x
	-

	
	08
	30“
	TC
	2“
	EPDM
	x
	-

	
	08
	30“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	x

	
	08
	30“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	x

	
	08
	30“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	-

	
	08
	30“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	-

	
	08
	40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	x

	
	08
	40“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	x

	
	08
	40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	-

	
	08
	40“
	DIN 11851 Male Part
	DN 50
	EPDM
	x
	-

	
	08
	40“
	TC
	2“
	Silicone
	x
	x

	
	08
	40“
	TC
	2“
	EPDM
	x
	x

	
	08
	40“
	TC
	2“
	Silicone
	x
	-

	
	08
	40“
	TC
	2“
	EPDM
	x
	-

	
	08
	40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	x

	
	08
	40“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	x

	
	08
	40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	-

	
	08
	40“
	Welding Stubs
	50.8 x 1.65
	EPDM
	x
	-













XX = 25 (Adapter 25 / code 7)	20
XX = 28 (Sartorius Adapter 28 tripple Bayonet)
FILTER SERIES 810 - 08-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	V-BAND
	AISI 304
	
	1

	3
	CARTRIDGE PLATE
	AISI 316L
	
	1

	4
	O-RING d=5.35 ID=266.06
	SILICONE
	
	1

	5
	GASKET CLAMP
	PTFE
	
	2

	6
	BEND FLANGE
	AISI 304
	
	4

	7
	INLET BEND
	AISI 316L
	
	1

	8
	OUTLET BEND
	AISI 316L
	
	1

	9
	COMPLETE LEG
	AISI 304
	
	3

	11
	PROTECTION PLATE
	AISI 316L
	
	1


[image: ]
FILTER SERIES 810 - 08-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	R mm
	S mm
	N mm
	C mm
	E mm
	VOLUME liters (V)
	PED Category

	12 x 10“
	425
	410
	279
	930
	290
	41
	II

	12 x 20“
	425
	410
	279
	1180
	540
	66
	II

	12 x 30“
	425
	410
	279
	1430
	790
	88
	II

	12 x 40“
	425
	410
	279
	1680
	1040
	112
	III



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	2.5“ (63.5mm x 1.65mm)
	326
	493
	225
	326
	573
	225



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	DN65
	326
	547
	252
	326
	627
	252



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.5“ (63.5mm x 1.65mm)
	326
	467
	212
	326
	547
	212



	PACKAGING SIZE AND WEIGHT
	

	CARTRIDGE x HEIGHT (N)
	BOWL WEIGHT [kg]
	TOTAL NET WEIGHT [kg]
	PACKAGING SIZE [cm]
	TOTAL WEIGHT PACKED [kg]
	

	12 x 10“
	10.0
	58.0
	75x53x54
	63.0
	

	12 x 20“
	14.5
	62.0
	100x53x54
	67.0
	

	12 x 30“
	19.0
	66.0
	125x53x54
	71.0
	

	12 x 40“
	23.5
	70.0
	150x53x54
	76.0
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	12
	30“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x

	
	12
	30“
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	x

	
	12
	30“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-

	
	12
	30“
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	-

	
	12
	30“
	TC
	2.5“
	Silicone
	x
	x

	
	12
	30“
	TC
	2.5“
	EPDM
	x
	x

	
	12
	30“
	TC
	2.5“
	Silicone
	x
	-

	
	12
	30“
	TC
	2.5“
	EPDM
	x
	-

	
	12
	30“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	x

	
	12
	30“
	Welding Stubs
	63.5 x 1.65
	EPDM
	x
	x

	
	12
	30“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	-

	
	12
	30“
	Welding Stubs
	63.5 x 1.65
	EPDM
	x
	-

	
	12
	40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x

	
	12
	40“
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	x

	
	12
	40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-

	
	12
	40“
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	-

	
	12
	40“
	TC
	2.5“
	Silicone
	x
	x

	
	12
	40“
	TC
	2.5“
	EPDM
	x
	x

	
	12
	40“
	TC
	2.5“
	Silicone
	x
	-

	
	12
	40“
	TC
	2.5“
	EPDM
	x
	-

	
	12
	40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	x

	
	12
	40“
	Welding Stubs
	63.5 x 1.65
	EPDM
	x
	x

	
	12
	40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	-

	
	12
	40“
	Welding Stubs
	63.5 x 1.65
	EPDM
	x
	-
























XX = 25 (Adapter 25 / code 7)	24
XX = 28 (Sartorius Adapter 28 tripple Bayonet)
[image: ]FILTER SERIES 810 - 12-ROUND LIQUID HOUSING
HOUSING STYLE - T-TYPE - Series VHP
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	BOLT CLAMP M16
	AISI 316Ti
	
	

	3
	O-RING d=7.00 ID=342.30
	SILICONE
	
	1

	4
	CARTRIDGE PLATE
	AISI 316L
	
	1

	5
	LEG
	AISI 304
	
	3

	6
	FOOT
	AISI 304
	
	3

	7
	CLAMP 3“
	AISI 304
	
	2

	8.1
	GASKET CLAMP 3“
	PTFE
	
	2

	8.2
	O-RING d=5.34 ID=100.00
	SILICONE
	
	2

	9
	INLET BEND
	AISI 316L
	
	1

	10
	OUTLET BEND
	AISI 316L
	
	1

	11
	PROTECTION PLATE
	AISI 316L
	
	1


[image: ]
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	R mm
	S mm
	N mm
	C mm
	E mm
	VOLUME liters (V)
	PED Category

	18 x 10“
	505
	480
	304
	950
	290
	54
	II

	18 x 20“
	505
	480
	304
	1200
	540
	85
	II

	18 x 30“
	505
	480
	304
	1450
	790
	115
	III

	18 x 40“
	505
	480
	304
	1700
	1040
	146
	III



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	2.5“ (63.5mm x 1.65mm) [Standard]
	325
	509
	225
	325
	589
	225

	3.0“ (76.2mm x 1.65mm)
	297
	565
	253
	297
	645
	253



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	DN65 [Standard]
	325
	564
	252
	325
	644
	252

	DN80
	316
	620
	276
	316
	700
	276



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.5“ (63.5mm x 1.65mm) [Standard]
	325
	482
	212
	325
	565
	212

	3.0“ (76.2mm x 1.65mm)
	297
	540
	240
	297
	620
	240



	PACKAGING SIZE AND WEIGHT

	CARTRIDGE x HEIGHT (N)
	BOWL WEIGHT [kg]
	TOTAL NET WEIGHT [kg]
	PACKAGING SIZE [cm]
	TOTAL WEIGHT PACKED [kg]

	18 x 10“
	12.0
	59.0
	78x58x59
	64.0

	18 x 20“
	17.0
	63.0
	103x58x59
	68.0

	18 x 30“
	22.0
	68.0
	128x58x59
	74.0

	18 x 40“
	27.0
	74.0
	153x58x59
	80.0
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“
	Standard Dimension

	
	18
	30“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x
	x

	
	18
	30“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x
	

	
	18
	30“
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	x
	x

	
	18
	30“
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	x
	

	
	18
	30“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-
	x

	
	18
	30“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-
	

	
	18
	30“
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	-
	x

	
	18
	30“
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	-
	

	
	18
	30“
	TC
	2.5“
	Silicone
	x
	x
	x

	
	18
	30“
	TC
	3.0“
	Silicone
	x
	x
	

	
	18
	30“
	TC
	2.5“
	EPDM
	x
	x
	x

	
	18
	30“
	TC
	3.0“
	EPDM
	x
	x
	

	
	18
	30“
	TC
	2.5“
	Silicone
	x
	-
	x

	
	18
	30“
	TC
	3.0“
	Silicone
	x
	-
	

	
	18
	30“
	TC
	2.5“
	EPDM
	x
	-
	x

	
	18
	30“
	TC
	3.0“
	EPDM
	x
	-
	

	
	18
	30“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	x
	x

	
	18
	30“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x
	

	
	18
	30“
	Welding Stubs
	63.5 x 1.65
	EPDM
	x
	x
	x

	
	18
	30“
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	x
	

	
	18
	30“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	-
	x

	
	18
	30“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-
	

	
	18
	30“
	Welding Stubs
	63.5 x 1.65
	EPDM
	x
	-
	x

	
	18
	30“
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	-
	

	
	18
	40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x
	x

	
	18
	40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x
	

	
	18
	40“
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	x
	x

	
	18
	40“
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	x
	

	
	18
	40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-
	x

	
	18
	40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-
	

	
	18
	40“
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	-
	x

	
	18
	40“
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	-
	

	
	18
	40“
	TC
	2.5“
	Silicone
	x
	x
	x

	
	18
	40“
	TC
	3.0“
	Silicone
	x
	x
	

	
	18
	40“
	TC
	2.5“
	EPDM
	x
	x
	x

	
	18
	40“
	TC
	3.0“
	EPDM
	x
	x
	

	
	18
	40“
	TC
	2.5“
	Silicone
	x
	-
	x

	
	18
	40“
	TC
	3.0“
	Silicone
	x
	-
	

	
	18
	40“
	TC
	2.5“
	EPDM
	x
	-
	x

	
	18
	40“
	TC
	3.0“
	EPDM
	x
	-
	

	
	18
	40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	x
	x

	
	18
	40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x
	

	
	18
	40“
	Welding Stubs
	63.5 x 1.65
	EPDM
	x
	x
	x

	
	18
	40“
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	x
	

	
	18
	40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	-
	x

	
	18
	40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-
	

	
	18
	40“
	Welding Stubs
	63.5 x 1.65
	EPDM
	x
	-
	x

	
	18
	40“
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	-
	


XX = 25 (Adapter 25 / code 7)	28
XX = 28 (Sartorius Adapter 28 tripple Bayonet)





	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	BOLT CLAMP M16
	AISI 316Ti
	
	

	3
	O-RING d=7.00 ID=393.10
	SILICONE
	
	1

	4
	CARTRIDGE PLATE
	AISI 316L
	
	1

	5
	LEG
	AISI 304
	
	3

	6
	FOOT
	AISI 304
	
	3

	7
	CLAMP 3“
	AISI 304
	
	2

	8.1
	GASKET CLAMP 3“
	PTFE
	
	2

	8.2
	O-RING d=5.34 ID=110.50
	SILICONE
	
	2

	9
	INLET BEND
	AISI 316L
	
	1

	10
	OUTLET BEND
	AISI 316L
	
	1

	11
	PROTECTION PLATE
	AISI 316L
	
	1



[image: ]
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	R mm
	S mm
	N mm
	C mm
	E mm
	VOLUME liters (V)
	PED Category

	24 x 10“
	465
	455
	-
	970
	290
	73
	II

	24 x 20“
	465
	455
	-
	1220
	540
	112
	II

	24 x 30“
	465
	455
	-
	1470
	790
	151
	III

	24 x 40“
	465
	455
	-
	1720
	1040
	190
	III



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	2.5“ (63.5mm x 1.65mm) [Standard]
	318
	509
	563
	318
	643
	264

	3.0“ (76.2mm x 1.65mm)
	292
	578
	252
	292
	660
	252

	4.0“ ( 101.6mm x 2.11mm)
	300
	566
	245
	300
	647
	245



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	DN65 [Standard]
	318
	618
	291
	318
	698
	291

	DN80
	331
	616
	295
	331
	696
	295

	DN100
	300
	638
	281
	300
	718
	281



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.5“ (63.5mm x 1.65mm) [Standard]
	318
	539
	252
	318
	518
	252

	3.0“ (76.2mm x 1.65mm)
	292
	554
	239
	292
	547
	239

	DN4“ (101.6mm x 2.11mm)
	300
	534
	229
	300
	603
	229



	PACKAGING SIZE AND WEIGHT

	CARTRIDGE x HEIGHT (N)
	BOWL WEIGHT [kg]
	TOTAL NET WEIGHT [kg]
	PACKAGING SIZE [cm]
	TOTAL WEIGHT PACKED [kg]

	24 x 10“
	18.0
	88.0
	80x63x64
	95.0

	24 x 20“
	27.0
	97.0
	105x63x64
	105.0

	24 x 30“
	35.0
	105.0
	130x63x64
	113.0

	24 x 40“
	44.0
	114.0
	155x63x64
	122.0
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“
	Standard Dimension

	
	24
	30"
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x
	x

	
	24
	30"
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x
	

	
	24
	30"
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	x
	

	
	24
	30"
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	x
	x

	
	24
	30"
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	x
	

	
	24
	30"
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	x
	

	
	24
	30"
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-
	x

	
	24
	30"
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-
	

	
	24
	30"
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	-
	

	
	24
	30"
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	-
	x

	
	24
	30"
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	-
	

	
	24
	30"
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	-
	

	
	24
	30"
	TC
	2,5"
	Silicone
	x
	x
	x

	
	24
	30"
	TC
	3"
	Silicone
	x
	x
	

	
	24
	30"
	TC
	4"
	Silicone
	x
	x
	

	
	24
	30"
	TC
	2,5"
	EPDM
	x
	x
	x

	
	24
	30"
	TC
	3"
	EPDM
	x
	x
	

	
	24
	30"
	TC
	4"
	EPDM
	x
	x
	

	
	24
	30"
	TC
	2,5"
	Silicone
	x
	-
	x

	
	24
	30"
	TC
	3"
	Silicone
	x
	-
	

	
	24
	30"
	TC
	4"
	Silicone
	x
	-
	

	
	24
	30"
	TC
	2,5"
	EPDM
	x
	-
	x

	
	24
	30"
	TC
	3"
	EPDM
	x
	-
	

	
	24
	30"
	TC
	4"
	EPDM
	x
	-
	

	
	24
	30"
	Welding Stubs
	63,5 x 1.65
	Silicone
	x
	x
	x

	
	24
	30"
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x
	

	
	24
	30"
	Welding Stubs
	101.6 x 2.11
	Silicone
	x
	x
	

	
	24
	30"
	Welding Stubs
	63,5 x 1.65
	EPDM
	x
	x
	x

	
	24
	30"
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	x
	

	
	24
	30"
	Welding Stubs
	101.6 x 2.11
	EPDM
	x
	x
	

	
	24
	30"
	Welding Stubs
	63,5 x 1.65
	Silicone
	x
	-
	x

	
	24
	30"
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-
	

	
	24
	30"
	Welding Stubs
	101.6 x 2.11
	Silicone
	x
	-
	

	
	24
	30"
	Welding Stubs
	63,5 x 1.65
	EPDM
	x
	-
	x

	
	24
	30"
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	-
	

	
	24
	30"
	Welding Stubs
	101.6 x 2.11
	EPDM
	x
	-
	




XX = 25 (Adapter 25 / code 7)
XX = 28 (Sartorius Adapter 28 tripple Bayonet)
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“
	Standard Dimension

	
	24
	40"
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x
	x

	
	24
	40"
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x
	

	
	24
	40"
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	x
	

	
	24
	40"
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	x
	x

	
	24
	40"
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	x
	

	
	24
	40"
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	x
	

	
	24
	40"
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-
	x

	
	24
	40"
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-
	

	
	24
	40"
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	-
	

	
	24
	40"
	DIN 11851 Male Part
	DN 65
	EPDM
	x
	-
	x

	
	24
	40"
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	-
	

	
	24
	40"
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	-
	

	
	24
	40"
	TC
	2,5"
	Silicone
	x
	x
	x

	
	24
	40"
	TC
	3"
	Silicone
	x
	x
	

	
	24
	40"
	TC
	4"
	Silicone
	x
	x
	

	
	24
	40"
	TC
	2,5"
	EPDM
	x
	x
	x

	
	24
	40"
	TC
	3"
	EPDM
	x
	x
	

	
	24
	40"
	TC
	4"
	EPDM
	x
	x
	

	
	24
	40"
	TC
	2,5"
	Silicone
	x
	-
	x

	
	24
	40"
	TC
	3"
	Silicone
	x
	-
	

	
	24
	40"
	TC
	4"
	Silicone
	x
	-
	

	
	24
	40"
	TC
	2,5"
	EPDM
	x
	-
	x

	
	24
	40"
	TC
	3"
	EPDM
	x
	-
	

	
	24
	40"
	TC
	4"
	EPDM
	x
	-
	

	
	24
	40"
	Welding Stubs
	63,5 x 1.65
	Silicone
	x
	x
	x

	
	24
	40"
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x
	

	
	24
	40"
	Welding Stubs
	101.6 x 2.11
	Silicone
	x
	x
	

	
	24
	40"
	Welding Stubs
	63,5 x 1.65
	EPDM
	x
	x
	x

	
	24
	40"
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	x
	

	
	24
	40"
	Welding Stubs
	101.6 x 2.11
	EPDM
	x
	x
	

	
	24
	40"
	Welding Stubs
	63,5 x 1.65
	Silicone
	x
	-
	x

	
	24
	40"
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-
	

	
	24
	40"
	Welding Stubs
	101.6 x 2.11
	Silicone
	x
	-
	

	
	24
	40"
	Welding Stubs
	63,5 x 1.65
	EPDM
	x
	-
	x

	
	24
	40"
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	-
	

	
	24
	40"
	Welding Stubs
	101.6 x 2.11
	EPDM
	x
	-
	




XX = 25 (Adapter 25 / code 7)
XX = 28 (Sartorius Adapter 28 tripple Bayonet)
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	BOLT CLAMP M16
	AISI 316Ti
	
	

	3
	O-RING d=7.00 ID=443.40
	SILICONE
	
	1

	4
	CARTRIDGE PLATE
	AISI 316L
	
	1

	5
	LEG
	AISI 304
	
	4

	6
	FOOT
	AISI 304
	
	4

	7
	CLAMP 4“
	AISI 304
	
	2

	8.1
	GASKET CLAMP 4“
	PTFE
	
	2

	8.2
	O-RING d=5.34 ID=136.50
	SILICONE
	
	2

	9
	INLET BEND
	AISI 316L
	
	1

	10
	OUTLET BEND
	AISI 316L
	
	1

	11
	PROTECTION PLATE
	AISI 316L
	
	1


[image: ]
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[image: ]Fluid group 1 (dangerous) on request
article no., price u delivery time can be different.
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	R mm
	S mm
	N mm
	C mm
	E mm
	VOLUME liters (V)
	PED Category

	30 x 10“
	550
	550
	-
	1000
	290
	118
	III

	30 x 20“
	550
	550
	-
	1250
	540
	176
	III

	30 x 30“
	550
	550
	-
	1500
	790
	235
	III

	30 x 40“
	550
	550
	-
	1750
	1040
	293
	III



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	3.0“ (76.2mm x 1.65mm) [Standard]
	292
	685
	323
	292
	765
	323

	4.0“ ( 101.6mm x 2.11mm)
	300
	662
	306
	30
	742
	306




	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	Q
	A
	L
	Q

	DN80 [Standard]
	331
	712
	356
	331
	792
	356

	DN100
	300
	734
	342
	300
	814
	342




	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	3.0“ (76.2mm x 1.65mm) [Standard]
	292
	660
	310
	292
	740
	310

	DN 4.0“ (101.6mm x 2.11mm)
	300
	630
	290
	300
	710
	290




	PACKAGING SIZE AND WEIGHT

	CARTRIDGE x HEIGHT (N)
	BOWL WEIGHT [kg]
	TOTAL NET WEIGHT [kg]
	PACKAGING SIZE [cm]
	TOTAL WEIGHT PACKED [kg]

	30 x 10“
	28.0
	93.0
	80x100x78
	112.0

	30 x 20“
	38.0
	101.0
	105x100x78
	121.0

	30 x 30“
	48.0
	109.0
	130x100x78
	131.0

	30 x 40“
	58.0
	117.0
	155x100x78
	140.0
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“
	Standard Dimension

	
	30
	30“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x
	x

	
	30
	30“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	x
	

	
	30
	30“
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	x
	x

	
	30
	30“
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	x
	

	
	30
	30“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-
	x

	
	30
	30“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	-
	

	
	30
	30“
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	-
	x

	
	30
	30“
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	-
	

	
	30
	30“
	TC
	3.0“
	Silicone
	x
	x
	x

	
	30
	30“
	TC
	4.0“
	Silicone
	x
	x
	

	
	30
	30“
	TC
	3.0“
	EPDM
	x
	x
	x

	
	30
	30“
	TC
	4.0“
	EPDM
	x
	x
	

	
	30
	30“
	TC
	3.0“
	Silicone
	x
	-
	x

	
	30
	30“
	TC
	4.0“
	Silicone
	x
	-
	

	
	30
	30“
	TC
	3.0“
	EPDM
	x
	-
	x

	
	30
	30“
	TC
	4.0“
	EPDM
	x
	-
	

	
	30
	30“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x
	x

	
	30
	30“
	Welding Stubs
	101.6 x 1.65
	Silicone
	x
	x
	

	
	30
	30“
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	x
	x

	
	30
	30“
	Welding Stubs
	101.6 x 1.65
	EPDM
	x
	x
	

	
	30
	30“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-
	x

	
	30
	30“
	Welding Stubs
	101.6 x 1.65
	Silicone
	x
	-
	

	
	30
	30“
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	-
	x

	
	30
	30“
	Welding Stubs
	101.6 x 1.65
	EPDM
	x
	-
	

	
	30
	40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x
	x

	
	30
	40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	x
	

	
	30
	40“
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	x
	x

	
	30
	40“
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	x
	

	
	30
	40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-
	x

	
	30
	40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	-
	

	
	30
	40“
	DIN 11851 Male Part
	DN 80
	EPDM
	x
	-
	x

	
	30
	40“
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	-
	

	
	30
	40“
	TC
	3.0“
	Silicone
	x
	x
	x

	
	30
	40“
	TC
	4.0“
	Silicone
	x
	x
	

	
	30
	40“
	TC
	3.0“
	EPDM
	x
	x
	x

	
	30
	40“
	TC
	4.0“
	EPDM
	x
	x
	

	
	30
	40“
	TC
	3.0“
	Silicone
	x
	-
	x

	
	30
	40“
	TC
	4.0“
	Silicone
	x
	-
	

	
	30
	40“
	TC
	3.0“
	EPDM
	x
	-
	x

	
	30
	40“
	TC
	4.0“
	EPDM
	x
	-
	

	
	30
	40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x
	x

	
	30
	40“
	Welding Stubs
	101.6 x 1.65
	Silicone
	x
	x
	

	
	30
	40“
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	x
	x

	
	30
	40“
	Welding Stubs
	101.6 x 1.65
	EPDM
	x
	x
	

	
	30
	40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-
	x

	
	30
	40“
	Welding Stubs
	101.6 x 1.65
	Silicone
	x
	-
	

	
	30
	40“
	Welding Stubs
	76.2 x 1.65
	EPDM
	x
	-
	x

	
	30
	40“
	Welding Stubs
	101.6 x 1.65
	EPDM
	x
	-
	


XX = 25 (Adapter 25 / code 7)	37
XX = 28 (Sartorius Adapter 28 tripple Bayonet)





	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	BOLT CLAMP M16
	AISI 316Ti
	
	

	3
	O-RING d=7.00 ID=532.30
	SILICONE
	
	1

	4
	CARTRIDGE PLATE
	AISI 316L
	
	1

	5
	LEG
	AISI 304
	
	4

	6
	FOOT
	AISI 304
	
	4

	7
	CLAMP 4“
	AISI 304
	
	2

	8.1
	GASKET CLAMP 4“
	PTFE
	
	2

	8.2
	O-RING d=5.34 ID=164.46
	SILICONE
	
	2

	9
	INLET BEND
	AISI 316L
	
	1

	10
	OUTLET BEND
	AISI 316L
	
	1

	11
	PROTECTION PLATE
	AISI 316L
	-
	1
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Fluid group 1 (dangerous) on request
article no., price u delivery time can be differ.TECHNICHAL DATA
VESSEL RANGE
PRM
NO. CARTRIDGED x HEIGHT
36 x 30“
CARTRIDGE SOCKET
226 CODE 7
ATEX REGULATION
GROUP 2 - Cat 2 GASuDUST FLUID GR IIC zone 1u21
DESIGN CODE
DIN EN 13445
CERTIFICATION
PED 2014/68/EU
PED CATEGORY
III
DESIGN PRESSURE -20°C +40°C (PS)
-1bar...+10bar
DESIGN PRESSURE -20°C +150°C (PS)
-1bar...+4bar
DESIGN TEMP. MIN-MAX (TS)
-20°C...+150°C
VESSEL MATERIAL
316L / 1.4404
TEST PRESSURE (PT)
20 bar
TOTAL VESSEL VOLUME liters (V)
235
FLUIDGROUP
2
PHYSICAL STATE
LIQUID / GAS
SEALS MATERIAL
SILICONE
INTERNAL FINISH
MECHANICAL POLISHING
INTERNAL ROUGHNESS
RA <0.8 MICRON
EXTERNAL FINISH
MECHANICAL POLISHING
VENT CONNECTION	A
CLAMP ASME 1.5“
IN/OUT CONNECTION B
DIN11851-DN100 MALE PART
DRAIN CONNECTION C
CLAMP ASME 1.5“
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“
	Standard Diameter

	
	36
	30“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	-
	x

	
	36
	30“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	x
	

	
	36
	30“
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	-
	x

	
	36
	30“
	DIN 11851 Male Part
	DN 100
	EPDM
	x
	x
	








































XX = 25 (Adapter 25 / code 7)	40
XX = 28 (Sartorius Adapter 28 tripple Bayonet)





Type 810
Fluid group 1 (dangerous) Series SH
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	C mm
	E mm
	VOLUME liters (V)
	PED Category
	Fluid Group

	01 x 10“
	790
	300
	3.0
	I
	1 (dangerous)

	01 x 20“
	1040
	550
	4.8
	I
	1 (dangerous)

	01 x 30“
	1290
	800
	6.7
	II
	1 (dangerous)

	01 x 40“
	1540
	1050
	8.6
	II
	1 (dangerous)



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.0“ (25.4mm x 1.65mm)
	375
	189
	104
	375
	270
	154

	1.5“ (38,1mm x 1.65mm)
	355
	220
	122
	355
	370
	198



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	DN25 (25.4mm x 1.65mm)
	375
	221
	120
	375
	302
	170

	DN40 (38,1mm x 1.65mm)
	355
	258
	144
	355
	415
	217

	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	P
	A
	L
	P

	1.0“ (25.4mm x 1.65mm)
	375
	163
	91
	375
	244
	141

	1.5“ (38.1mm x 1.65mm)
	355
	194
	112
	355
	345
	185



	SMS MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.0“ (25.4mm x 1.65mm)
	375
	203
	111
	375
	284
	161

	1.5“ (38,1mm x 1.65mm)
	355
	240
	133
	355
	391
	208




43




	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.0“

	
	01
	10“-40“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	x

	
	01
	10“-40“
	DIN 11851 Male Part
	DN 25
	Silicone
	x
	-

	
	01
	10“-40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	x

	
	01
	10“-40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	-

	
	01
	10“-40“
	TC
	1“
	Silicone
	x
	x

	
	01
	10“-40“
	TC
	1.5“
	Silicone
	x
	-

	
	01
	10“-40“
	TC
	1“
	Silicone
	x
	x

	
	01
	10“-40“
	TC
	1.5“
	Silicone
	x
	-

	
	01
	10“-40“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	x

	
	01
	10“-40“
	Welding Stubs
	381. x 1.65
	Silicone
	x
	-

	
	01
	10“-40“
	Welding Stubs
	25.4 x 1.65
	Silicone
	x
	x

	
	01
	10“-40“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	-

	
	01
	10“-40“
	SMS - Male part
	25.4 x 1.65
	Silicone
	x
	x

	
	01
	10“-40“
	SMS - Male part
	381. x 1.65
	Silicone
	x
	-

	
	01
	10“-40“
	SMS - Male part
	25.4 x 1.65
	Silicone
	x
	x

	
	01
	10“-40“
	SMS - Male part
	38.1 x 1.65
	Silicone
	x
	-




„X“ = Placeholder for the bowl height:

1 = 10“
2 = 20“
3 = 30“
4 = 40“
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	CLAMP 4“
	AISI 304
	
	1

	3
	CARFTRIDGES PLATE + BENDS
	AISI 316L
	
	1

	4
5
	GASKET CLAMP 4“
	SILICONE
	
	1

	
	LEG
	AISI 304
	
	3





[image: ]
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	C mm
	E mm
	VOLUME liters (V)
	PED Category
	Fluid Group

	03 x 10“
	816
	290
	7.3
	II
	1 (dangerous)

	03 x 20“
	1065
	540
	12.6
	II
	1 (dangerous)

	03 x 30“
	1314
	790
	17.8
	II
	1 (dangerous)

	03 x 40“
	1564
	1040
	23.1
	III
	1 (dangerous)



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.5“ (38.1mm x 1.65mm)
	345
	310
	148
	345
	385
	223



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	DN40 (38.1mm x 1.65mm)
	345
	351
	168
	345
	426
	243



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	P
	A
	L
	P

	1.5“ (38.1mm x 1.65mm)
	345
	285
	135
	345
	360
	210



	SMS MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.5“ (38,1mm x 1.65mm)
	345
	331
	158
	345
	406
	233









Please Note
In filter housings with a flange connection at the in- and outlet e.g. DIN-EN1092-1, ANSI, etc. the bends will be welded directly to the baseplate, instead of the standard flange connection described in the detailed drawing.
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	03
	10“-40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	x

	
	03
	10“-40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	-

	
	03
	10“-40“
	TC
	1.5“
	Silicone
	x
	x

	
	03
	10“-40“
	TC
	1.5“
	Silicone
	x
	-

	
	03
	10“-40“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	x

	
	03
	10“-40“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	-

	
	03
	10“-40“
	SMS - Male part
	38.1 x 1.65
	Silicone
	x
	x

	
	03
	10“-40“
	SMS - Male part
	38.1 x 1.65
	Silicone
	x
	-



„X“ = Placeholder for the bowl height:

1 = 10“
2 = 20“
3 = 30“
4 = 40“
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	V-BAND
	AISI 304
	
	1

	3
	CARTRIDGE PLATE
	AISI 316L
	
	1

	4
	O-RING d=5.35 ID=158.11
	SILICONE
	
	1

	5
	GASKET CLAMP 1.5“
	PTFE
	
	2

	6
	BEND FLANGE
	AISI 304
	
	4

	7
	INLET BEND
	AISI 316L
	
	1

	8
	OUTLET BEND
	AISI 316L
	
	1

	9
	COMPLETE LEG
	AISI 304
	
	3

	11
	PROTECTION PLATE
	AISI 316L
	
	1
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	C mm
	E mm
	VOLUME liters (V)
	PED Category
	Fluid Group

	05 x 10“
	825
	290
	11
	II
	1 (dangerous)

	05 x 20“
	1075
	540
	20
	II
	1 (dangerous)

	05 x 30“
	1325
	790
	29.1
	III
	1 (dangerous)

	05 x 40“
	1575
	1040
	38.2
	III
	1 (dangerous)



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.5“ (38.1mm x 1.65mm)
	345
	331
	168
	345
	406
	243

	2.0“ (50.8mm x 1.65mm)
	315
	379
	196
	315
	446
	263



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	DN40 (38.1mm x 1.65mm)
	345
	371
	188
	345
	446
	263

	DN50 (50.8mm x 1.65mm)
	315
	423
	218
	315
	490
	285



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	P
	A
	L
	P

	1.5“ (38.1mm x 1.65mm)
	345
	305
	155
	345
	380
	230

	2.0“ (50.8mm x 1.65mm)
	315
	353
	183
	315
	420
	250



	SMS MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.5“ (38,1mm x 1.65mm)
	345
	351
	178
	345
	426
	253

	2.0“ (50.8mm x 1.65mm)
	315
	403
	208
	315
	470
	275




Please Note
In filter housings with a flange connection at the in- and outlet e.g. DIN-EN1092-1, ANSI, etc. the bends will be welded directly to the baseplate, instead of the standard flange connection described in the detailed drawing.
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	05
	10“-40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	x

	
	05
	10“-40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	-

	
	05
	10“-40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	x

	
	05
	10“-40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	-

	
	05
	10“-40“
	TC
	1.5“
	Silicone
	x
	x

	
	05
	10“-40“
	TC
	1.5“
	Silicone
	x
	-

	
	05
	10“-40“
	TC
	2“
	Silicone
	x
	x

	
	05
	10“-40“
	TC
	2“
	Silicone
	x
	-

	
	05
	10“-40“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	x

	
	05
	10“-40“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	-

	
	05
	10“-40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	x

	
	05
	10“-40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	-

	
	05
	10“-40“
	SMS - Male part
	381. x 1.65
	Silicone
	x
	x

	
	05
	10“-40“
	SMS - Male part
	381. x 1.65
	Silicone
	x
	-

	
	05
	10“-40“
	SMS - Male part
	50.8 x 1.65
	Silicone
	x
	x

	
	05
	10“-40“
	SMS - Male part
	50.8 x 1.65
	Silicone
	x
	-



„X“ = Placeholder for the bowl height:

1 = 10“
2 = 20“
3 = 30“
4 = 40“
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	V-BAND
	AISI 304
	
	1

	3
	CARTRIDGE PLATE
	AISI 316L
	
	1

	4
	O-RING d=5.35 ID=208.91
	SILICONE
	
	1

	5
	GASKET CLAMP 2“
	PTFE
	
	2

	6
	BEND FLANGE
	AISI 304
	
	4

	7
	INLET BEND
	AISI 316L
	
	1

	8
	OUTLET BEND
	AISI 316L
	
	1

	9
	COMPLETE LEG
	AISI 304
	
	3

	11
	PROTECTION PLATE
	AISI 316L
	
	1
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	C mm
	E mm
	VOLUME liters (V)
	PED Category
	Fluid Group

	08 x 10“
	846
	290
	21.3
	III
	1 (dangerous)

	08 x 20“
	1096
	540
	35.5
	III
	1 (dangerous)

	08 x 30“
	1346
	790
	49.7
	III
	1 (dangerous)

	08 x 40“
	1596
	1040
	63.9
	III
	1 (dangerous)



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.5“ (38.1mm x 1.65mm)
	345
	357
	194
	345
	432
	269

	2.0“ (50.8mm x 1.65mm)
	315
	405
	222
	315
	472
	289

	2.5“ (63.5mm x 1.65mm)
	286
	468
	243
	286
	548
	323

	3.0“ (76.2mm x 1.65mm)
	258
	524
	271
	258
	604
	351



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	DN40 (38.1mm x 1.65mm)
	345
	397
	214
	345
	472
	289

	DN50 (50.8mm x 1.65mm)
	315
	449
	244
	315
	516
	311

	DN65 (63.5mm x 1.65mm)
	286
	518
	268
	286
	602
	350

	DN80 (76.2mm x 1.65mm)
	258
	588
	303
	258
	658
	383



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	P
	A
	L
	P

	1.5“ (38.1mm x 1.65mm)
	345
	331
	181
	345
	406
	256

	2.0“ (50.8mm x 1.65mm)
	315
	379
	209
	315
	446
	276

	2.5“ (63.5mm x 1.65mm)
	286
	442
	230
	286
	522
	310

	3.0“ (76.2mm x 1.65mm)
	258
	498
	258
	258
	578
	338



	SMS - Male part

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	1.5“ (38.1mm x 1.65mm)
	345
	377
	204
	345
	452
	279

	2.0“ (50.8mm x 1.65mm)
	315
	429
	234
	315
	496
	301

	2.5“ (63.5mm x 1.65mm)
	286
	502
	260
	286
	582
	340

	3.0“ (76.2mm x 1.65mm)
	258
	568
	293
	258
	648
	373



Please Note
In filter housings with a flange connection at the in- and outlet e.g. DIN-EN1092-1, ANSI, etc. the bends will be welded directly to the baseplate, instead of the standard flange connection described in the detailed drawing.
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	08
	10“-40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	x

	
	08
	10“-40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	-

	
	08
	10“-40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	x

	
	08
	10“-40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	-

	
	08
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x

	
	08
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-

	
	08
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x

	
	08
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-

	
	08
	10“-40“
	TC
	1.5“
	Silicone
	x
	x

	
	08
	10“-40“
	TC
	1.5“
	Silicone
	x
	-

	
	08
	10“-40“
	TC
	2“
	Silicone
	x
	x

	
	08
	10“-40“
	TC
	2“
	Silicone
	x
	-

	
	08
	10“-40“
	TC
	2.5“
	Silicone
	x
	x

	
	08
	10“-40“
	TC
	2.5“
	Silicone
	x
	-

	
	08
	10“-40“
	TC
	3.0“
	Silicone
	x
	x

	
	08
	10“-40“
	TC
	3.0“
	Silicone
	x
	-

	
	08
	10“-40“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	x

	
	08
	10“-40“
	Welding Stubs
	38.1 x 1.65
	Silicone
	x
	-

	
	08
	10“-40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	x

	
	08
	10“-40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	-

	
	08
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	x

	
	08
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	-

	
	08
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x

	
	08
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-

	
	08
	10“-40“
	SMS - Male part
	38.1 x 1.65
	Silicone
	x
	x

	
	08
	10“-40“
	SMS - Male part
	38.1 x 1.65
	Silicone
	x
	-

	
	08
	10“-40“
	SMS - Male part
	50.8 x 1.65
	Silicone
	x
	x

	
	08
	10“-40“
	SMS - Male part
	50.8 x 1.65
	Silicone
	x
	-

	
	08
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	x

	
	08
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	-

	
	08
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	x

	
	08
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	-



„X“ = Placeholder for the bowl height:

1 = 10“
2 = 20“
3 = 30“
4 = 40“
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	V-BAND
	AISI 304
	
	1

	3
	CARTRIDGE PLATE
	AISI 316L
	
	1

	4
	O-RING d=5.35 ID=266.06
	SILICONE
	
	1

	5
	GASKET CLAMP
	PTFE
	
	2

	6
	BEND FLANGE
	AISI 304
	
	4

	7
	INLET BEND
	AISI 316L
	-
	1

	8
	OUTLET BEND
	AISI 316L
	-
	1

	9
	COMPLETE LEG
	AISI 304
	-
	3

	11
	PROTECTION PLATE
	AISI 316L
	-
	1
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	C mm
	E mm
	VOLUME liters (V)
	PED Category
	Fluid Group

	12 x 10“
	930
	290
	41
	III
	1 (dangerous)

	12 x 20“
	1180
	540
	66
	III
	1 (dangerous)

	12 x 30“
	1430
	790
	89
	III
	1 (dangerous)

	12 x 40“
	1680
	1040
	113
	IV
	1 (dangerous)



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.0“ (50.8mm x 1.65mm)
	350
	474
	238
	350
	544
	238

	2.5“ (63.5mm x 1.65mm)
	326
	493
	225
	326
	573
	225

	3.0“ (76.2mm x 1.65mm)
	298
	549
	253
	298
	629
	253

	4.0“ (101.6mm x 2mm)
	290
	529
	243
	290
	609
	243



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	DN50 (50.8mm x 1.65mm)
	350
	519
	258
	350
	586
	258

	DN65 (63.5mm x 1.65mm)
	326
	547
	252
	326
	627
	252

	DN80 (76.2mm x 1.65mm)
	297
	603
	280
	297
	683
	280

	DN100 (101.6mm x 2mm)
	290
	527
	202
	290
	687
	282



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	P
	A
	L
	P

	2.0“ (50.8mm x 1.65mm)
	350
	449
	225
	350
	518
	225

	2.5“ (63.5mm x 1.65mm)
	326
	467
	212
	326
	547
	212

	3.0“ (76.2mm x 1.65mm)
	298
	523
	240
	298
	603
	240

	4.0“ (101.6mm x 2mm)
	290
	483
	210
	290
	583
	230



	SMS - Male part

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.0“ (50.8mm x 1.65mm)
	350
	499
	250
	350
	568
	250

	2.5“ (63.5mm x 1.65mm)
	326
	527
	242
	326
	607
	242

	3.0“ (76.2mm x 1.65mm)
	298
	593
	275
	298
	673
	275

	4.0“ (101.6mm x 2mm)
	290
	543
	240
	290
	643
	260
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	12
	10“-40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	x

	
	12
	10“-40“
	DIN 11851 Male Part
	DN 50
	Silicone
	x
	-

	
	12
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x

	
	12
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-

	
	12
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x

	
	12
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-

	
	12
	10“-40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	x

	
	12
	10“-40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	-

	
	12
	10“-40“
	TC
	2.0“
	Silicone
	x
	x

	
	12
	10“-40“
	TC
	2.0“
	Silicone
	x
	-

	
	12
	10“-40“
	TC
	2.5“
	Silicone
	x
	x

	
	12
	10“-40“
	TC
	2.5“
	Silicone
	x
	-

	
	12
	10“-40“
	TC
	3.0“
	Silicone
	x
	x

	
	12
	10“-40“
	TC
	3.0“
	Silicone
	x
	-

	
	12
	10“-40“
	TC
	4.0“
	Silicone
	x
	x

	
	12
	10“-40“
	TC
	4.0“
	Silicone
	x
	-

	
	12
	10“-40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	x

	
	12
	10“-40“
	Welding Stubs
	50.8 x 1.65
	Silicone
	x
	-

	
	12
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	x

	
	12
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	-

	
	12
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x

	
	12
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-

	
	12
	10“-40“
	Welding Stubs
	101.6 x 2.00
	Silicone
	x
	x

	
	12
	10“-40“
	Welding Stubs
	101.6 x 2.00
	Silicone
	x
	-

	
	12
	10“-40“
	SMS - Male part
	50.8 x 1.65
	Silicone
	x
	x

	
	12
	10“-40“
	SMS - Male part
	50.8 x 1.65
	Silicone
	x
	-

	
	12
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	x

	
	12
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	-

	
	12
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	x

	
	12
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	-

	
	12
	10“-40“
	SMS - Male part
	101.6 x 2.00
	Silicone
	x
	x

	
	12
	10“-40“
	SMS - Male part
	101.6 x 2.00
	Silicone
	x
	-








„X“ = Placeholder for the bowl height:

1 = 10“
2 = 20“
3 = 30“
4 = 40“
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	-
	1

	2
	BOLT CLAMP M16
	AISI 316Ti
	
	

	3
	O-RING d=7.00 ID=342.30
	SILICONE
	
	1

	4
	CARTRIDGE PLATE
	AISI 316L
	
	1

	5
	LEG
	AISI 304
	
	3

	6
	FOOT
	AISI 304
	
	3

	7
	CLAMP 3“
	AISI 304
	
	2

	8.1
	GASKET CLAMP 3“
	PTFE
	
	2

	8.2
	O-RING d=5.34 ID=100.00
	SILICONE
	-
	2

	9
	INLET BEND
	AISI 316L
	-
	1

	10
	OUTLET BEND
	AISI 316L
	-
	1

	11
	PROTECTION PLATE
	AISI 316L
	-
	1
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	C mm
	E mm
	VOLUME liters (V)
	PED Category
	Fluid Group

	18 x 10“
	950
	290
	54
	III
	1 (dangerous)

	18 x 20“
	1200
	540
	85
	III
	1 (dangerous)

	18 x 30“
	1450
	790
	115
	III
	1 (dangerous)

	18 x 40“
	1700
	1040
	146
	IV
	1 (dangerous)



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.5“ (63.5mm x 1.65mm)
	325
	509
	225
	325
	589
	225

	3.0“ (76.2mm x 1.65mm)
	297
	566
	253
	297
	646
	253

	4.0“ (101.6mm x 2mm)
	287
	552
	246
	287
	632
	246



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	DN65
	325
	564
	252
	325
	644
	252

	DN80
	296
	620
	280
	296
	700
	280

	DN100
	287
	604
	262
	287
	704
	282



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	P
	A
	L
	P

	2.5“ (63.5mm x 1.65mm)
	325
	484
	212
	325
	564
	212

	3.0“ (76.2mm x 1.65mm)
	297
	540
	240
	297
	620
	240

	4.0“ (101.6mm x 2mm)
	292
	604
	314
	292
	600
	230



	SMS - Male part

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.5“ (63.5mm x 1.65mm)
	325
	544
	242
	325
	624
	242

	3.0“ (76.2mm x 1.65mm)
	297
	610
	275
	297
	690
	275

	4.0“ (101.6mm x 2mm)
	287
	580
	260
	287
	660
	260




63




	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	18
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x

	
	18
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-

	
	18
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x

	
	18
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-

	
	18
	10“-40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	x

	
	18
	10“-40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	-

	
	18
	10“-40“
	TC
	2.5“
	Silicone
	x
	x

	
	18
	10“-40“
	TC
	2.5“
	Silicone
	x
	-

	
	18
	10“-40“
	TC
	3.0“
	Silicone
	x
	x

	
	18
	10“-40“
	TC
	3.0“
	Silicone
	x
	-

	
	18
	10“-40“
	TC
	4.0“
	Silicone
	x
	x

	
	18
	10“-40“
	TC
	4.0“
	Silicone
	x
	-

	
	18
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	x

	
	18
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	-

	
	18
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x

	
	18
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-

	
	18
	10“-40“
	Welding Stubs
	101.6 x 2.00
	Silicone
	x
	x

	
	18
	10“-40“
	Welding Stubs
	101.6 x 2.00
	Silicone
	x
	-

	
	18
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	x

	
	18
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	-

	
	18
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	x

	
	18
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	-

	
	18
	10“-40“
	SMS - Male part
	101.6 x 2.00
	Silicone
	x
	x

	
	18
	10“-40“
	SMS - Male part
	101.6 x 2.00
	Silicone
	x
	-




„X“ = Placeholder for the bowl height:

1 = 10“
2 = 20“
3 = 30“
4 = 40“
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	BOLT CLAMP M16
	AISI 316Ti
	
	

	3
	O-RING d=7.00 ID=393.10
	SILICONE
	
	1

	4
	CARTRIDGE PLATE
	AISI 316L
	
	1

	5
	LEG
	AISI 304
	
	3

	6
	FOOT
	AISI 304
	
	3

	7
	CLAMP 3“
	AISI 304
	
	2

	8.1
	GASKET CLAMP 3“
	PTFE
	
	2

	8.2
	O-RING d=5.34 ID=110.50
	SILICONE
	
	2

	9
	INLET BEND
	AISI 316L
	
	1

	10
	OUTLET BEND
	AISI 316L
	-
	1

	11
	PROTECTION PLATE
	AISI 316L
	-
	1
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	C mm
	E mm
	VOLUME liters (V)
	PED Category
	Fluid Group

	24 x 10“
	970
	290
	73
	III
	1 (dangerous)

	24 x 20“
	1220
	540
	112
	III
	1 (dangerous)

	24 x 30“
	1470
	790
	151
	IV
	1 (dangerous)

	24 x 40“
	1720
	1040
	190
	IV
	1 (dangerous)



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.5“ (63.5mm x 1.65mm)
	318
	564
	265
	318
	644
	265

	3.0“ (76.2mm x 1.65mm)
	292
	580
	253
	292
	660
	253

	4.0“ ( 101.6mm x 2.11mm)
	300
	566
	245
	300
	647
	246



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	DN65 (63.5mm x 1.65mm)
	318
	618
	292
	318
	698
	292

	DN80 (85mm x 2mm)
	331
	616
	296
	331
	696
	296

	DN100 (101.6mm x 2mm)
	300
	638
	281
	300
	718
	296

	DN125 (129.0mm x 2mm)
	253
	701
	314
	-
	-
	-



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	P
	A
	L
	P

	2.5“ (63.5mm x 1.65mm)
	318
	538
	252
	318
	618
	252

	3.0“ (76.2mm x 1.65mm)
	292
	554
	240
	292
	634
	240

	4.0“ (101.6mm x 2mm)
	300
	534
	229
	300
	614
	230

	5.0“ (139.7mm x 2.60mm)
	248
	615
	271
	-
	-
	-



	SMS - Male part

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.5“ (63.5mm x 1.65mm)
	318
	598
	282
	318
	678
	282

	3.0“ (76.2mm x 1.65mm)
	292
	624
	275
	292
	704
	275

	4.0“ (101.6mm x 2mm)
	300
	594
	259
	300
	674
	259
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Dia- meter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	24
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x

	
	24
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-

	
	24
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x

	
	24
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-

	
	24
	10“-40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	x

	
	24
	10“-40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	-

	
	24
	10“-40“
	DIN 11851 Male Part
	DN 125
	Silicone
	x
	-

	
	24
	10“-40“
	TC
	2.5“
	Silicone
	x
	x

	
	24
	10“-40“
	TC
	2.5“
	Silicone
	x
	-

	
	24
	10“-40“
	TC
	3.0“
	Silicone
	x
	x

	
	24
	10“-40“
	TC
	3.0“
	Silicone
	x
	-

	
	24
	10“-40“
	TC
	4.0“
	Silicone
	x
	x

	
	24
	10“-40“
	TC
	4.0“
	Silicone
	x
	-

	
	24
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	x

	
	24
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	-

	
	24
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x

	
	24
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-

	
	24
	10“-40“
	Welding Stubs
	101.6 x 2.00
	Silicone
	x
	x

	
	24
	10“-40“
	Welding Stubs
	101.6 x 2.00
	Silicone
	x
	-

	
	24
	10“-40“
	Welding Stubs
	139.7 x 2.60
	Silicone
	x
	-

	
	24
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	x

	
	24
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	-

	
	24
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	x

	
	24
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	-

	
	24
	10“-40“
	SMS - Male part
	101.6 x 2.00
	Silicone
	x
	x

	
	24
	10“-40“
	SMS - Male part
	101.6 x 2.00
	Silicone
	x
	-




„X“ = Placeholder for the bowl height:

1 = 10“
2 = 20“
3 = 30“
4 = 40“
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	BOLT CLAMP M16
	AISI 316Ti
	
	

	3
	O-RING d=7.00 ID=443.40
	SILICONE
	
	1

	4
	CARTRIDGE PLATE
	AISI 316L
	
	1

	5
	LEG
	AISI 304
	
	4

	6
	FOOT
	AISI 304
	
	4

	7
	CLAMP 4“
	AISI 304
	
	2

	8.1
	GASKET CLAMP 4“
	PTFE
	
	2

	8.2
	O-RING d=5.34 ID=136.50
	SILICONE
	
	2

	9
	INLET BEND
	AISI 316L
	
	1

	10
	OUTLET BEND
	AISI 316L
	
	1

	11
	PROTECTION PLATE
	AISI 316L
	-
	1
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	C mm
	E mm
	VOLUME liters (V)
	PED Category
	Fluid Group

	30 x 10“
	1000
	290
	118
	III
	1 (dangerous)

	30 x 20“
	1250
	540
	176
	III
	1 (dangerous)

	30 x 30“
	1500
	790
	235
	III
	1 (dangerous)

	30 x 40“
	1750
	1040
	293
	III
	1 (dangerous)



	CLAMP

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.5“ (63.5mm x 1.65mm)
	318
	665
	330
	318
	745
	330

	3.0“ (76.2mm x 1.65mm)
	291
	686
	323
	291
	766
	323

	4.0“ ( 101.6mm x 2.11mm)
	300
	662
	306
	300
	742
	306



	DIN 11851 MALE PART

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	DN65 (63.5mm x 1.65mm)
	318
	719
	357
	318
	800
	357

	DN80 (85mm x 2mm)
	331
	712
	356
	331
	792
	357

	DN100 (101.6mm x 2mm)
	300
	734
	342
	300
	814
	342

	DN125 (129.0mm x 2mm)
	254
	785
	362
	-
	-
	-

	DN150 (154.0mm x 2mm)
	218
	820
	355
	-
	-
	-



	BUTT WELD ASME BPE

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	L
	P
	A
	L
	P

	2.5“ (63.5mm x 1.65mm)
	318
	639
	317
	318
	719
	317

	3.0“ (76.2mm x 1.65mm)
	291
	660
	310
	291
	740
	310

	4.0“ (101.6mm x 2mm)
	300
	630
	290
	300
	710
	290

	5.0“ (139.7mm x 2.60mm)
	251
	671
	291
	-
	-
	-

	6.0“ (168.3mm x 2.60mm)
	210
	747
	329
	-
	-
	-



	SMS - Male part

	
	WITHOUT DRAIN
	WITH DRAIN

	Dimension [mm]
	A
	B
	Q
	A
	B
	Q

	2.5“ (63.5mm x 1.65mm)
	318
	699
	347
	318
	779
	347

	3.0“ (76.2mm x 1.65mm)
	291
	730
	345
	291
	810
	345

	4.0“ (101.6mm x 2mm)
	300
	690
	320
	300
	770
	320
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Dia- meter
	Gasket
	With Vent TC 1.5“
	With Drain TC 1.5“

	
	30
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	x

	
	30
	10“-40“
	DIN 11851 Male Part
	DN 65
	Silicone
	x
	-

	
	30
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	x

	
	30
	10“-40“
	DIN 11851 Male Part
	DN 80
	Silicone
	x
	-

	
	30
	10“-40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	x

	
	30
	10“-40“
	DIN 11851 Male Part
	DN 100
	Silicone
	x
	-

	
	30
	10“-40“
	DIN 11851 Male Part
	DN 125
	Silicone
	x
	-

	
	30
	10“-40“
	DIN 11851 Male Part
	DN 150
	Silicone
	x
	-

	
	30
	10“-40“
	TC
	2.5“
	Silicone
	x
	x

	
	30
	10“-40“
	TC
	2.5“
	Silicone
	x
	-

	
	30
	10“-40“
	TC
	3.0“
	Silicone
	x
	x

	
	30
	10“-40“
	TC
	3.0“
	Silicone
	x
	-

	
	30
	10“-40“
	TC
	4.0“
	Silicone
	x
	x

	
	30
	10“-40“
	TC
	4.0“
	Silicone
	x
	-

	
	30
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	x

	
	30
	10“-40“
	Welding Stubs
	63.5 x 1.65
	Silicone
	x
	-

	
	30
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	x

	
	30
	10“-40“
	Welding Stubs
	76.2 x 1.65
	Silicone
	x
	-

	
	30
	10“-40“
	Welding Stubs
	101.6 x 2.00
	Silicone
	x
	x

	
	30
	10“-40“
	Welding Stubs
	101.6 x 2.00
	Silicone
	x
	-

	
	30
	10“-40“
	Welding Stubs
	139.7 x 2.60
	Silicone
	x
	-

	
	30
	10“-40“
	Welding Stubs
	168.3 x 2.60
	Silicone
	x
	-

	
	30
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	x

	
	30
	10“-40“
	SMS - Male part
	63.5 x 1.65
	Silicone
	x
	-

	
	30
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	x

	
	30
	10“-40“
	SMS - Male part
	76.2 x 1.65
	Silicone
	x
	-

	
	30
	10“-40“
	SMS - Male part
	101.6 x 2.00
	Silicone
	x
	x

	
	30
	10“-40“
	SMS - Male part
	101.6 x 2.00
	Silicone
	x
	-




„X“ = Placeholder for the bowl height:

1 = 10“
2 = 20“
3 = 30“
4 = 40“
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	BOLT CLAMP M16
	AISI 316Ti
	
	

	3
	O-RING d=7.00 ID=532.30
	SILICONE
	
	1

	4
	CARTRIDGE PLATE
	AISI 316L
	
	1

	5
	LEG
	AISI 304
	
	4

	6
	FOOT
	AISI 304
	
	4

	7
	CLAMP 4“
	AISI 304
	
	2

	8.1
	GASKET CLAMP 4“
	PTFE
	
	2

	8.2
	O-RING d=5.34 ID=164.46
	SILICONE
	
	2

	9
	INLET BEND
	AISI 316L
	
	1

	10
	OUTLET BEND
	AISI 316L
	
	1

	11
	PROTECTION PLATE
	AISI 316L
	-
	1
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	TECHNICHAL DATA

	NO. CARTRIDGED
	01

	CARTRIDGE SOCKET
	226 CODE 7

	ATEX REGULATION
	GROUP 2 - Cat 2 GASuDUST FLUID GR IIC zone 1u21

	DESIGN CODE
	DIN EN 13445

	CERTIFICATION
	PED 2014/68/EU

	PED CATEGORY
	4.3

	DESIGN PRESSURE
	+10bar

	DESIGN TEMPERATURE
	-20°C...+150°C

	VESSEL MATERIAL
	316L / 1.4404

	FLUIDGROUP
	2 (not dangerous)

	PHYSICAL STATE
	LIQUID / GAS

	INTERNAL FINISH
	MECHANICAL POLISHING

	INTERNAL ROUGHNESS
	RA <0.8 MICRON

	EXTERNAL FINISH
	MECHANICAL POLISHING

	INLET CONNECTION	A
	CLAMP ASME 1.5“ (38.1mm x 1.65xx)

	OUTLET CONNECTION B
	CLAMP ASME 1.5“ (38.1mm x 1.65xx)

	DRAIN CONNECTION	C
	CLAMP ASME 0.5“ (12.7mm x 1.65xx)





[image: ]DIMENSIONAL DATA
CARTRIDGE x HEIGHT (N)
A mm
B mm
PED Category
01 x 05“
272
227
4.3
01 x 10“
375
333
4.3
01 x 20“
625
581
4.3
01 x 30“
875
831
4.3

SPARE PARTS
DESCRIPTION
MATERIAL
PART NO.
Q.TY
CLAMP 4“
AISI 304

1
GASKET 4“
SILICONE

1
GASKET 4“
EPDM

1




	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection Inlet u Outlet
	Nominal Diameter
	Gasket
	With Drain TC 0.5“

	
	01
	05“
	TC
	1.5“
	Silicone
	x

	
	01
	10“
	TC
	1.5“
	Silicone
	x

	
	01
	20“
	TC
	1.5“
	Silicone
	x

	
	01
	30“
	TC
	1.5“
	Silicone
	x

	
	01
	05“
	TC
	1.5“
	EPDM
	x

	
	01
	10“
	TC
	1.5“
	EPDM
	x

	
	01
	20“
	TC
	1.5“
	EPDM
	x

	
	01
	30“
	TC
	1.5“
	EPDM
	x
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Type 810 - Gas 1-round Housings
(10 bar Version)
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	C [mm] with Vent u Drain BSPF 1/4“ female
	C [mm] with Vent TC 1.5“ u Drain TC 0.5“
	B [mm] with Drain BSPF 1/4“ female
	B [mm] with Drain TC 0.5“
	PED Category

	01 x 5“
	381
	381
	178
	168
	4.3

	01 x 10“
	501
	501
	178
	168
	4.3

	01 x 20“
	751
	751
	178
	168
	4.3

	01 x 30“
	1001
	1001
	178
	168
	I

	01 x 40“
	1251
	1251
	178
	168
	I



	CLAMP

	Dimension
	L [mm]
	Q [mm]
	N [mm]

	1.5“ (38.1mm x 1.65mm)
	129
	62
	99




	DIN 11851 MALE PART

	Dimension
	L [mm]
	Q [mm]
	N [mm]

	DN40
	188
	81
	99




	BUTT WELD ASME BPE

	Dimension
	L [mm]
	Q [mm]
	N [mm]

	1.5“ (38.1mm x 1.65mm)
	264
	129
	99




	PACKAGING SIZE AND WEIGHT

	CARTRIDGE x HEIGHT (N)
	BOWL WEIGHT [kg]
	TOTAL NET WEIGHT [kg]
	TOTAL WEIGHT PACKED [kg]

	01 x 5“
	0.7
	2.6
	3.6

	01 x 10“
	1.1
	3.0
	4.0

	01 x 20“
	1.9
	4.0
	5.0

	01 x 30“
	2.7
	5.0
	6.0

	01 x 40“
	3.5
	6.0
	7.0
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection
	Nominal Diameter
	Gasket
	With Vent u Drain BSPF 1/4“ female [G/H]
	With Vent TC 1.5“ u Drain TC 0.5“
[G/H]

	
	01
	5“
	TC
	1.5“
	Silicone
	x
	

	
	01
	5“
	TC
	1.5“
	EPDM
	x
	

	
	01
	5“
	Welding Stubs
	1.5“
	Silicone
	x
	

	
	01
	5“
	Welding Stubs
	1.5“
	EPDM
	x
	

	
	01
	5“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	

	
	01
	5“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	

	
	01
	10“
	TC
	1.5“
	Silicone
	x
	

	
	01
	10“
	TC
	1.5“
	EPDM
	x
	

	
	01
	10“
	Welding Stubs
	1.5“
	Silicone
	x
	

	
	01
	10“
	Welding Stubs
	1.5“
	EPDM
	x
	

	
	01
	10“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	

	
	01
	10“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	

	
	01
	20“
	TC
	1.5“
	Silicone
	x
	

	
	01
	20“
	TC
	1.5“
	EPDM
	x
	

	
	01
	20“
	Welding Stubs
	1.5“
	Silicone
	x
	

	
	01
	20“
	Welding Stubs
	1.5“
	EPDM
	x
	

	
	01
	20“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	

	
	01
	20“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	

	
	01
	30“
	TC
	1.5“
	Silicone
	x
	

	
	01
	30“
	TC
	1.5“
	EPDM
	x
	

	
	01
	30“
	Welding Stubs
	1.5“
	Silicone
	x
	

	
	01
	30“
	Welding Stubs
	1.5“
	EPDM
	x
	

	
	01
	30“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	

	
	01
	30“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	

	
	01
	40“
	TC
	1.5“
	Silicone
	x
	

	
	01
	40“
	TC
	1.5“
	EPDM
	x
	

	
	01
	40“
	Welding Stubs
	1.5“
	Silicone
	x
	

	
	01
	40“
	Welding Stubs
	1.5“
	EPDM
	x
	

	
	01
	40“
	DIN 11851 Male Part
	DN 40
	Silicone
	x
	

	
	01
	40“
	DIN 11851 Male Part
	DN 40
	EPDM
	x
	

	
	01
	5“
	TC
	1.5“
	Silicone
	
	x

	
	01
	5“
	TC
	1.5“
	EPDM
	
	x

	
	01
	10“
	TC
	1.5“
	Silicone
	
	x

	
	01
	10“
	TC
	1.5“
	EPDM
	
	x

	
	01
	20“
	TC
	1.5“
	Silicone
	
	x

	
	01
	20“
	TC
	1.5“
	EPDM
	
	x

	
	01
	30“
	TC
	1.5“
	Silicone
	
	x

	
	01
	30“
	TC
	1.5“
	EPDM
	
	x

	
	01
	40“
	TC
	1.5“
	Silicone
	
	x

	
	01
	40“
	TC
	1.5“
	EPDM
	
	x
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	SPARE PARTS

	POS.
	DESCRIPTION
	MATERIAL
	PART NO.
	Q.TY

	1
	HOUSING BOWL
	AISI 316L
	
	1

	2
	CLAMP 3.5“
	AISI 304
	
	1

	
4
	GASKET CLAMP 3.5“
	SILICONE
	
	1

	
	GASKET CLAMP 3.5“
	EPDM
	
	1






[image: ]
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Type 805 - Gas Multi-round Housings
(5 bar Version)
[image: ]
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	FASTENING SYTEM
	De [mm]
	C
[mm]
	K [mm]
	CONNECTIONS DN
max /  max mm
	TOTAL VOLUME [L]
	PED Category

	03 x 10“
	
V


V


R
	
219


273


320
	829
	
443


511


515
	DN 100 /  114.3mm
DN 125 /  139.7mm DN 125 /  139.7mm
	33
	I

	03 x 20“
	
	
	1079
	
	
	42
	II

	05 x 10“
	
	
	875
	
	
	46
	II

	05 x 20“
	
	
	1125
	
	
	61
	II

	08 x 10“
	
	
	935
	
	
	59
	II

	08 x 20“
	
	
	1175
	
	
	82
	II
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Heigh t
	Connection
	Nominal Diameter
	Gasket
	With Vent u Drain BSPF 1/2“
female
	With Vent u Drain TC 1.5“
	Standard

	
	03
	10“
	FLANGE DIN EN 1092-1
	DN 100
	Silicone
	x
	
	x

	
	03
	10“
	FLANGE DIN EN 1092-1
	DN 100
	EPDM
	x
	
	

	
	03
	20“
	FLANGE DIN EN 1092-1
	DN 100
	Silicone
	x
	
	x

	
	03
	20“
	FLANGE DIN EN 1092-1
	DN 100
	EPDM
	x
	
	

	
	05
	10“
	FLANGE DIN EN 1092-1
	DN 125
	Silicone
	x
	
	x

	
	05
	10“
	FLANGE DIN EN 1092-1
	DN 125
	EPDM
	x
	
	

	
	05
	20“
	FLANGE DIN EN 1092-1
	DN 125
	Silicone
	x
	
	x

	
	05
	20“
	FLANGE DIN EN 1092-1
	DN 125
	EPDM
	x
	
	

	
	08
	10“
	FLANGE DIN EN 1092-1
	DN 125
	Silicone
	x
	
	x

	
	08
	10“
	FLANGE DIN EN 1092-1
	DN 125
	EPDM
	x
	
	

	
	08
	20“
	FLANGE DIN EN 1092-1
	DN 125
	Silicone
	x
	
	x

	
	08
	20“
	FLANGE DIN EN 1092-1
	DN 125
	EPDM
	x
	
	

	
	03
	10“
	FLANGE DIN EN 1092-1
	DN 100
	Silicone
	
	x
	x

	
	03
	10“
	FLANGE DIN EN 1092-1
	DN 100
	EPDM
	
	x
	

	
	03
	20“
	FLANGE DIN EN 1092-1
	DN 100
	Silicone
	
	x
	x

	
	03
	20“
	FLANGE DIN EN 1092-1
	DN 100
	EPDM
	
	x
	

	
	05
	10“
	FLANGE DIN EN 1092-1
	DN 125
	Silicone
	
	x
	x

	
	05
	10“
	FLANGE DIN EN 1092-1
	DN 125
	EPDM
	
	x
	

	
	05
	20“
	FLANGE DIN EN 1092-1
	DN 125
	Silicone
	
	x
	x

	
	05
	20“
	FLANGE DIN EN 1092-1
	DN 125
	EPDM
	
	x
	

	
	08
	10“
	FLANGE DIN EN 1092-1
	DN 125
	Silicone
	
	x
	x

	
	08
	10“
	FLANGE DIN EN 1092-1
	DN 125
	EPDM
	
	x
	

	
	08
	20“
	FLANGE DIN EN 1092-1
	DN 125
	Silicone
	
	x
	x

	
	08
	20“
	FLANGE DIN EN 1092-1
	DN 125
	EPDM
	
	x
	

	OTHER SIZES ON REQUEST
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Type 808 - industrial
1- round - liquid housing
[image: ]
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[image: ]TECHNICHAL DATA
NO. CARTRIDGED
01
CARTRIDGE SOCKET
25 (Code 7)
CERTIFICATION
PED 2014/68/EU - art. 4 / sec. 3
FLUID GROUP
GROUP 2 (not dangerous)
DESIGN PRESSURE 0°C-40°C
8.0 bar
DESIGN PRESSURE 150°C
6.2 bar
TEST PRESSURE (PT)
10.5 bar
VESSEL MATERIAL
316L / 1.4404
GASKET
SILICONE
INTERNAL FINISHING
PICKLED
INTERNAL FINISHING
MECHANICAL POLISHING
DRAIN CONNECTION H + M
BSP 1/4“ FEMALE
VENT CONNECTION G
BSP 1/4“ MALE
DISTANCE L (ADAPTER 25 - CODE 7)
110 mm
DISTANCE L (ADAPTER 21 - CODE 8)
98 mm
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (Y)
	C mm
	D mm
	E mm
	X mm
	Y mm
	VOLUME liters (V)
	BOWL WEIGHT (kg)
	TOTAL NET WEIGHT (kg)

	01 x 10“
	572
	382
	300
	440
	320
	1.8
	1.1
	4

	01 x 20“
	827
	637
	554
	695
	575
	3.3
	1.9
	4.8

	01 x 30“
	1082
	892
	808
	950
	830
	4.8
	2.7
	5.6

	01 x 40“
	1337
	1147
	1062
	1205
	1085
	6.3
	3.5
	6.4



	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Adapter
	Version
	Connection Inlet u Outlet
	Gasket

	
	01
	10“
	25 (Code 7)
	ADVANCED
	BSP 3/4“ FEMALE
	Silicone

	
	01
	20“
	25 (Code 7)
	ADVANCED
	BSP 3/4“ FEMALE
	Silicone

	
	01
	30“
	25 (Code 7)
	ADVANCED
	BSP 3/4“ FEMALE
	Silicone

	
	01
	10“
	25 (Code 7)
	ADVANCED
	BSP 1“ FEMALE
	Silicone

	
	01
	20“
	25 (Code 7)
	ADVANCED
	BSP 1“ FEMALE
	Silicone

	
	01
	30“
	25 (Code 7)
	ADVANCED
	BSP 1“ FEMALE
	Silicone

	
	01
	10“
	21 (Code 8)
	ADVANCED
	BSP 3/4“ FEMALE
	Silicone

	
	01
	20“
	21 (Code 8)
	ADVANCED
	BSP 3/4“ FEMALE
	Silicone

	
	01
	30“
	21 (Code 8)
	ADVANCED
	BSP 3/4“ FEMALE
	Silicone

	
	01
	10“
	21 (Code 8)
	ADVANCED
	BSP 1“ FEMALE
	Silicone

	
	01
	20“
	21 (Code 8)
	ADVANCED
	BSP 1“ FEMALE
	Silicone

	
	01
	30“
	21 (Code 8)
	ADVANCED
	BSP 1“ FEMALE
	Silicone
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Type 800 - Vent Housings
(Pressureless)
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	DIMENSIONAL DATA

	CARTRIDGE x HEIGHT (N)
	A [mm]
	B [mm]
	C [mm]
(height needed for removing the bell over the cartris- ges)
	D [mm]
	E [mm]
	HANDLES

	
	
	CLAMP ASME BPE
	DIN 11851 LINER
	
	
	
	

	01 x 10“
	315
	43
	59
	300
	88.9
	130
	NO

	01 x 20“
	565
	43
	59
	550
	88.9
	130
	NO

	01 x 30“
	815
	43
	59
	800
	88.9
	130
	NO

	

	03 x 10“
	351
	97
	127
	300
	219
	400
	NO

	03 x 20“
	601
	97
	127
	550
	219
	400
	YES

	03 x 30“
	851
	97
	127
	800
	219
	400
	YES

	

	05 x 10“
	345
	106
	133
	300
	219
	400
	NO

	05 x 20“
	595
	106
	133
	550
	219
	400
	YES

	05 x 30“
	845
	106
	133
	800
	219
	400
	YES

	

	08 x 10“
	349
	120
	147
	300
	273
	440
	NO

	08 x 20“
	599
	120
	147
	550
	273
	440
	YES

	08 x 30“
	849
	120
	147
	800
	273
	440
	YES
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	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection Type Nominal Diameter / Size

	
	
	
	Clamp ASME BPE
	DIN 11851 Liner

	
	01
	10“
	2“ (50.8mm x 1.65mm)
	

	
	01
	20“
	2“ (50.8mm x 1.65mm)
	

	
	01
	30“
	2“ (50.8mm x 1.65mm)
	

	
	03
	10“
	3“ (76.2mm x 1.65mm)
	

	
	03
	20“
	3“ (76.2mm x 1.65mm)
	

	
	03
	30“
	3“ (76.2mm x 1.65mm)
	

	
	05
	10“
	4“ (101.2mm x 2.11mm)
	

	
	05
	20“
	4“ (101.2mm x 2.11mm)
	

	
	05
	30“
	4“ (101.2mm x 2.11mm)
	

	
	08
	10“
	4“ (101.2mm x 2.11mm)
	

	
	08
	20“
	4“ (101.2mm x 2.11mm)
	

	
	08
	30“
	4“ (101.2mm x 2.11mm)
	

	
	01
	10“
	
	DN 50

	
	01
	20“
	
	DN 50

	
	01
	30“
	
	DN 50

	
	03
	10“
	
	DN 80

	
	03
	20“
	
	DN 80

	
	03
	30“
	
	DN 80

	
	05
	10“
	
	DN 100

	
	05
	20“
	
	DN 100

	
	05
	30“
	
	DN 100

	
	08
	10“
	
	DN 100

	
	08
	20“
	
	DN 100

	
	08
	30“
	
	DN 100

	OTHER SIZES ON REQUEST
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	TECHNICAL DATA

	Material
	316L

	Internal Surface
	Ra 0.8μm EP

	External Surface
	RA 1.6μm EP

	Sartorius Adapter
	40

	Qty. cartridge
	1

	Height
	10“, 20“ u 30“

	Connector
	DIN 11851



[image: ]Parts not in contact with the Medium are made by Stainless Steel 304. Jumbo vent housings are delivered with Certificates of the materials.









	ORDER CODE AND TECHNICAL EQUIPMENT

	Order-no.
	No. of Cartridges
	Bowl Height
	Connection Type

DIN 11851 Liner

	
	01
	10“
	DN 100 (104x2)

	
	01
	20“
	DN 100 (104x2)

	
	01
	30“
	DN 100 (104x2)
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VOLUME LITRES (V)

PRESSURE(PS) min-max at TS=20+40°C bar
PRESSURE(PS) min-max at TS=20+150°C bar
TEST PRESSURE(PT) bar 20

DESIGN TEMPERATURE (TS) min-max -20 +150°C

FLUID GROUP (Art,13 - 2014/68/EU) 2-NOT DANG,

VESSEL MATERIAL 316L/1.4404
PHISICAL STATE LIQUID / GAS
YEAR OF MANUFACTURE

VESSEL NUMBER

ATEX CLASSIFICATION 26D lic

ATEX CERTIFICATION 04,01 EX,02-X

CExxxx &





image38.jpeg
©101.6

339+5





image39.jpeg
TECHNICAL DATA

VESSEL MODEL

SH - SANITARY.

NO. CARTRIDGES

01

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP 1-2 (DANGEROUS AND NOT)
PED CATEGORY 1

DESIGN PRESSURE (PS) 10 bar

TEST PRESSURE (PT) 14.5 bar

VESSEL MATERIAL 316L /14404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0.8 MICRON

EXTERNAL FINISHING

MECHANICAL POLISHING

VENT CONNECTIOI CLAMP 15"

VESSEL TYPE SH011 | SHO012 | SHO13 | SH014
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 790 1040 1290 1540
E mm 300 550 800 1050
TOTAL VESSEL VOLUME litres (V) 30 48 6.7 86
BOWL WEIGHT kg 20 43 46 59
TOTAL NET WEIGHT kg 70 82 94 106
PACKAGING SIZE CM30x27x| 112 112 112 127
TOTAL WEIGHT PACKED kg 8.0 85 1.0 130

WORKING CONDITIONS 2014/68/EJ MAX PRESSURE bar

FLUID GROUP STATE |TEMPERAT.|SH011|SH012 | SHO013 | SH014
DANGEROUS |LIQUID 0-40°C 100 100 100 | 100
DANGEROUS |LIQUID 150°C T5 75 5 5
DANGEROUS |GAS/VAPOR| 0-40° C 100 | 100 74 58
DANGEROUS | GAS/VAPOR| 150 75 75 74 58
NOT DANGER. | LIQUID 0-40°C 100 100 | 100 | 100
NOT DANGER | LIQUID 150° C 75 15 5 75
NOT DANGER | GAS/VAPOR| 0 - 40° C 100 | 100 100 | 100
NOT DANGER | GAS/VAPOR| 150° C 75 75 75 75
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY
NO. CARTRIDGES 03

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP

1-2 (DANGEROUS AND NOT)

PED CATEGORY

DESIGN PRESSURE (PS) 10 bar
TEST PRESSURE (PT) 145 bar
VESSEL MATERIAL 316L / 1.4404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0.8 MICRON

EXTERNAL FINISHING

MECHANICAL POLISHING

VENT CONNECTIO! CLAMP 15"

VESSEL TYPE SHO031 | SH032 | SHO33 | SH034
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 816 1065 1314 1564
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 7.3 126 178 231
BOWL WEIGHT kg 40 6.0 8.0 100
TOTAL NET WEIGHT kg 174 194 214 234
PACKAGING SIZE CM40x40x| 75 100 116 138
TOTAL WEIGHT PACKED kg 230 25.0 270 290
WORKING CONDITIONS 2014/68/EU MAX PRESSURE bar
FLUID GROUP STATE |TEMPERAT.|SH031|SH032 | SH033 | SH034
DANGEROUS |LIQUID 0-40°C 100 | 100 100 | 100
DANGEROUS |LIQUID 150° C 75 75 75 75
DANGEROUS |GASNVAPOR| 0-150°C 6.8 39 28 21
NOT DANGER [LIQUID 0-40°C 100 | 100 100 | 100
NOT DANGER [ LIQUID 150° C 75 75 75 75
NOT DANGER | GAS/VAPOR| 0-40° C 100 | 100 10.0 86
NOT DANGER | GAS/VAPOR| 150° C 75 75 75 75
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY
NO. CARTRIDGES 03

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP

1-2 (DANGEROUS AND NOT)

PED CATEGORY

DESIGN PRESSURE (PS) 10 bar
TEST PRESSURE (PT) 145 bar
VESSEL MATERIAL 316L / 1.4404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0.8 MICRON

EXTERNAL FINISHING

MECHANICAL POLISHING

VENT CONNECTIO! CLAMP 15"

VESSEL TYPE SHO031 | SH032 | SHO33 | SH034
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 816 1065 1314 1564
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 7.3 126 178 231
BOWL WEIGHT kg 40 6.0 8.0 100
TOTAL NET WEIGHT kg 174 194 214 234
PACKAGING SIZE CM40x40x| 75 100 116 138
TOTAL WEIGHT PACKED kg 230 25.0 270 290
WORKING CONDITIONS 2014/68/EU MAX PRESSURE bar
FLUID GROUP STATE |TEMPERAT.|SH031|SH032 | SH033 | SH034
DANGEROUS |LIQUID 0-40°C 100 | 100 100 | 100
DANGEROUS |LIQUID 150° C 75 75 75 75
DANGEROUS |GASNVAPOR| 0-150°C 6.8 39 28 21
NOT DANGER [LIQUID 0-40°C 100 | 100 100 | 100
NOT DANGER [ LIQUID 150° C 75 75 75 75
NOT DANGER | GAS/VAPOR| 0-40° C 100 | 100 10.0 86
NOT DANGER | GAS/VAPOR| 150° C 75 75 75 75
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY
NO. CARTRIDGES 05

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP

1-2 (DANGEROUS AND NOT)

PED CATEGORY

DESIGN PRESSURE (PS) 10 bar
TEST PRESSURE (PT) 45 bar
VESSEL MATERIAL 316L / 1.4404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0.8 MICRON

EXTERNAL FINISHING

MECHANICAL POLISHING

VENT CONNECTION CLAMP 15"

VESSEL TYPE SHO51 | SHO052 | SHO53 | SH054
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 825 1075 1325 1575
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 1.0 200 291 382
BOWL WEIGHT kg 53 75 102 129
TOTAL NET WEIGHT kg 18.0 20.0 220 240
PACKAGING SIZE CM45x33x| 75 100 118 143
TOTAL WEIGHT PACKED kg 240 260 280 300
WORKING CONDITIONS 2014/68/EU MAX PRESSURE bar
FLUID GROUP STATE | TEMPERAT.|SH051 |SH052 | SH053 | SH054
DANGEROUS |LIQUID 0-40°C 100 | 100 100 | 100
DANGEROUS |LIQUID 150° C 5 15 75 75
DANGEROUS |GAS/VAPOR| 0-150° C 45 24 17 13
NOT DANGER | LIQUID 0-40°C 100 | 100 100 10.0
NOT DANGER.|LIQUID 150° C 75 75 T5 75
NOT DANGER.| GAS/VAPOR| 0 -40° C 100 99 6.8 52
NOT DANGER | GASIVAPOR| 150° C 15 75 68 52
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY
NO. CARTRIDGES 05

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP

1-2 (DANGEROUS AND NOT)

PED CATEGORY

DESIGN PRESSURE (PS) 10 bar
TEST PRESSURE (PT) 45 bar
VESSEL MATERIAL 316L / 1.4404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0.8 MICRON

EXTERNAL FINISHING

MECHANICAL POLISHING

VENT CONNECTION CLAMP 15"

VESSEL TYPE SHO51 | SHO052 | SHO53 | SH054
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 825 1075 1325 1575
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 1.0 200 291 382
BOWL WEIGHT kg 53 75 102 129
TOTAL NET WEIGHT kg 18.0 20.0 220 240
PACKAGING SIZE CM45x33x| 75 100 118 143
TOTAL WEIGHT PACKED kg 240 260 280 300
WORKING CONDITIONS 2014/68/EU MAX PRESSURE bar
FLUID GROUP STATE | TEMPERAT.|SH051 |SH052 | SH053 | SH054
DANGEROUS |LIQUID 0-40°C 100 | 100 100 | 100
DANGEROUS |LIQUID 150° C 5 15 75 75
DANGEROUS |GAS/VAPOR| 0-150° C 45 24 17 13
NOT DANGER | LIQUID 0-40°C 100 | 100 100 10.0
NOT DANGER.|LIQUID 150° C 75 75 T5 75
NOT DANGER.| GAS/VAPOR| 0 -40° C 100 99 6.8 52
NOT DANGER | GASIVAPOR| 150° C 15 75 68 52
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY
NO.CARTRIDGES 08

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP 1-2 (DANGEROUS AND NOT)

PED CATEGORY

]

DESIGN PRESSURE (PS) 10 bar
TEST PRESSURE (PT) 145 bar
VESSEL MATERIAL 316L /14404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0.8 MICRON

EXTERNAL FINISHI|

MECHANICAL POLISHING

VENT CONNECTIOI CLAMP 15"

VESSEL TYPE SHO081 | SH082 | SH083 | SH084
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 846 1096 1346 1596
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 213 355 497 639
BOWL WEIGHT kg 70 100 13.0 160
TOTAL NET WEIGHT kg 270 30.0 330 36.0
PACKAGING SIZE CM50x40x| 75 100 118 143
TOTAL WEIGHT PACKED kg 300 340 38.0 420

WORKING CONDITIONS 2014/68/EJMAX PRESSURE bar

FLUID GROUP STATE |TEMPERAT.|SH081|SH082 | SH083 | SH084
DANGEROUS |LIQUID 0-40°C 100 100 | 100 | 10.0
DANGEROUS |LIQUID 150°C 15 75 75 5
DANGEROUS |GAS/VAPOR| 0-150° C 23 14 10 07
NOT DANGER | LIQUID 0-40°C 100 100 100 | 100
NOT DANGER | LIQUID 150° C 75 75 75 75
NOT DANGER | GAS/VAPOR| 0 - 40° C 93 56 40 31
NOT DANGER | GAS/VAPOR| 150° C I5 56 4.0 3.1
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY
NO.CARTRIDGES 08

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP 1-2 (DANGEROUS AND NOT)

PED CATEGORY

]

DESIGN PRESSURE (PS) 10 bar
TEST PRESSURE (PT) 145 bar
VESSEL MATERIAL 316L /14404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0.8 MICRON

EXTERNAL FINISHI|

MECHANICAL POLISHING

VENT CONNECTIOI CLAMP 15"

VESSEL TYPE SHO081 | SH082 | SH083 | SH084
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 846 1096 1346 1596
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 213 355 497 639
BOWL WEIGHT kg 70 100 13.0 160
TOTAL NET WEIGHT kg 270 30.0 330 36.0
PACKAGING SIZE CM50x40x| 75 100 118 143
TOTAL WEIGHT PACKED kg 300 340 38.0 420

WORKING CONDITIONS 2014/68/EJMAX PRESSURE bar

FLUID GROUP STATE |TEMPERAT.|SH081|SH082 | SH083 | SH084
DANGEROUS |LIQUID 0-40°C 100 100 | 100 | 10.0
DANGEROUS |LIQUID 150°C 15 75 75 5
DANGEROUS |GAS/VAPOR| 0-150° C 23 14 10 07
NOT DANGER | LIQUID 0-40°C 100 100 100 | 100
NOT DANGER | LIQUID 150° C 75 75 75 75
NOT DANGER | GAS/VAPOR| 0 - 40° C 93 56 40 31
NOT DANGER | GAS/VAPOR| 150° C I5 56 4.0 3.1
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY
NO.CARTRIDGES 12

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP 1-2 (DANGEROUS AND NOT)
PED CATEGORY ]

DESIGN PRESSURE (PS 9.0 bar

TEST PRESSURE (PT) 13.0 bar

VESSEL MATERIAL 316L / 14404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0 8 MICRON

EXTERNAL FINISHING

MECHANICAL POLISHING

VENT CONNECTION CLAMP 15"

VESSEL TYPE SH121 | SH122 | SH123 | SH124
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 930 1180 1430 1680
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 41 66 89 113
BOWL WEIGHT kg 10 145 19 235
TOTAL NET WEIGHT kg 58 62 66 70
PACKAGING SIZE CM54x53x| 75 100 125 150
TOTAL WEIGHT PACKED kg 63 67 71 76

WORKING CONDITIONS 2014/68/EU MAX PRESSURE bar
FLUID GROUP STATE |TEMPERAT.|SH121|SH122 | SH123 | SH124
DANGEROUS |LIQUID 0-40°C 90 90 90 9.0
DANGEROUS |LIQUID 150° C 70 70 70 70
DANGEROUS |GAS/VAPOR| 0-150° C 12 07 05 05
NOT DANGER | LIQUID 0-40°C 90 9.0 9.0 9.0
NOT DANGER |LIQUID 150° C 70 70 7.0 70
NOT DANGER. | GAS/VAPOR| 0 - 150° C 48 30 22 17
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TECHNICAL DATA

VESSEL MODEL

SH - SANITARY.

NO. CARTRIDGES

18

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU
FLUID GROUP. 1-2 (DANGEROUS AND NOT)

PED CATEGORY

DESIGN PRESSURE (PS) 8 bar
TEST PRESSURE (PT) 11.5 bar
VESSEL MATERIAL 316L / 14404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0 8 MICRON

EXTERNAL FINISHIN(

MECHANICAL POLISHING

VENT CONNECTION CLAMP 1.5"

VESSEL TYPE SH181 | SH182 | SH183 | SH184
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 950 1200 1450 1700
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V] 54 85 115 146
BOWL WEIGHT kg 12 17 22 27
TOTAL NET WEIGHT kg 59 63 68 74
PACKAGING SIZE CM59x58x| 78 103 128 153
TOTAL WEIGHT PACKED kg 64 68 74 80

WORKING CONDITIONS 2014/68/EU MAX PRESSURE bar
FLUID GROUP STATE |TEMPERAT.|SH181|SH182 | SH183 | SH184
DANGEROUS |LIQUID 0-40°C 8.0 80 80 80
DANGEROUS |LIQUID 150° C 62 62 6.2 62
DANGEROUS |GAS/VAPOR| 0-150° C 09 05 05 05
NOT DANGER | LIQUID 0-40°C 80 80 8.0 80
NOT DANGER | LIQUID 150° C 62 62 6.2 62
NOT DANGER | GAS/VAPOR| 0 - 150° C 36 23 17 1.3
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY
NO.CARTRIDGES 24

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP 1-2 (DANGEROUS AND NOT)

PED CATEGORY

DESIGN PRESSURE (PS) 8 bar
TEST PRESSURE (PT) 11.5 bar
VESSEL MATERIAL 316L / 1.4404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0.8 MICRON

EXTERNAL FINISHING

MECHANICAL POLISHING

VENT CONNECTION CLAMP 15"

VESSEL TYPE SH241 | SH242 | SH243 | SH244
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 970 1220 1470 1720
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 73 12 151 190
BOWL WEIGHT kg 18 27 35 44
TOTAL NET WEIGHT kg 88 97 105 114
PACKAGING SIZE CMB4x63x| 80 105 130 155
TOTAL WEIGHT PACKED kg 95 105 113 122

WORKING CONDITIONS 2014/68/EJMAX PRESSURE bar

FLUID GROUP STATE |TEMPERAT.|SH241 |SH242 | SH243 | SH244
DANGEROUS |LIQUID 0-40°C 8.0 80 80 80
DANGEROUS |LIQUID 150° C 62 62 62 62
DANGEROUS |GAS/VAPOR| 0-150° C 27 1.7 13 10
NOT DANGER.|LIQUID 0-40°C 80 80 8.0 80
NOT DANGER | LIQUID 150° C 62 62 6.2 6.2
NOT DANGER | GAS/VAPOR| 0 -40° C 80 80 6.5 52
NOT DANGER | GAS/VAPOR| 150° C 6.2 62 6.2 52
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY.
NO. CARTRIDGES 30

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP.

1-2 (DANGEROUS AND NOT)

PED CATEGORY

DESIGN PRESSURE (PS) 8 bar
TEST PRESSURE (PT) 11.5 bar
VESSEL MATERIAL 316L / 14404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0 8 MICRON

EXTERNAL FINISHI|

MECHANICAL POLISHING

VENT CONNECTION CLAMP 15"

VESSEL TYPE SH301 | SH302 | SH303 | SH304
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 1000 1250 1500 1750
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 118 176 235 293
BOWL WEIGHT kg 28 38 48 58
TOTAL NET WEIGHT kg 93 101 109 17
PACKAGING SIZE CM78x100x| 80 105 130 155
TOTAL WEIGHT PACKED kg 112 121 131 140

WORKING CONDITIONS 2014/68/EJMAX PRESSURE bar

FLUID GROUP STATE |TEMPERAT.|SH301 |SH302 | SH303 | SH304
DANGEROUS |LIQUID 0-40°C 8.0 80 80 80
DANGEROUS |LIQUID 150°C 62 6.2 6.2 6.2
DANGEROUS | GAS/VAPOR| 0-150° C 16 1.1 08 06
NOT DANGER | LIQUID 0-4 80 80 8.0 80
NOT DANGER |LIQUID 150° C 62 62 6.2 62
NOT DANGER.| GAS/VAPOR| 0 -40° C 80 56 42 34
NOT DANGER | GAS/VAPOR| 150° C 62 56 42 34
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TECHNICAL DATA

VESSEL MODEL SH - SANITARY.
NO. CARTRIDGES 30

DESIGN CODE AD MERKBLATT
CERTIFICATION 2014/68/EU

FLUID GROUP.

1-2 (DANGEROUS AND NOT)

PED CATEGORY

DESIGN PRESSURE (PS) 8 bar
TEST PRESSURE (PT) 11.5 bar
VESSEL MATERIAL 316L / 14404

SEALS MATERIAL

SILICONE FDA BGA APPROVED

INTERNAL FINISHING

MECHANICAL POLISHING

INTERNAL ROUGHTNESS

RA<0 8 MICRON

EXTERNAL FINISHI|

MECHANICAL POLISHING

VENT CONNECTION CLAMP 15"

VESSEL TYPE SH301 | SH302 | SH303 | SH304
CARTRIDGES HEIGHT 10" 20" 30" 40"
C mm 1000 1250 1500 1750
E mm 290 540 790 1040
TOTAL VESSEL VOLUME litres (V) 118 176 235 293
BOWL WEIGHT kg 28 38 48 58
TOTAL NET WEIGHT kg 93 101 109 17
PACKAGING SIZE CM78x100x| 80 105 130 155
TOTAL WEIGHT PACKED kg 112 121 131 140

WORKING CONDITIONS 2014/68/EJMAX PRESSURE bar

FLUID GROUP STATE |TEMPERAT.|SH301 |SH302 | SH303 | SH304
DANGEROUS |LIQUID 0-40°C 8.0 80 80 80
DANGEROUS |LIQUID 150°C 62 6.2 6.2 6.2
DANGEROUS | GAS/VAPOR| 0-150° C 16 1.1 08 06
NOT DANGER | LIQUID 0-4 80 80 8.0 80
NOT DANGER |LIQUID 150° C 62 62 6.2 62
NOT DANGER.| GAS/VAPOR| 0 -40° C 80 56 42 34
NOT DANGER | GAS/VAPOR| 150° C 62 56 42 34
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@MD®  FILTER HOUSING

PART NUMBER

MODEL

TYPE

CARTRIDGE NO. x HIGH (inch)
CATEGORY 2014/68/EU

VOLUME LITRES (V)
PRESSURE(PS) min-max at TS=-20+150°C bar

TEST PRESSURE(PT) bar

DESIGN TEMPERATURE (TS) min-max -20+150°C

FLUID GROUP (Art.13 - 2014/68/EU)

VESSEL MATERIAL 316L / 1.4404
YEAR OF MANUFACTURE

VESSEL NUMBER

ATEX CLASSIFICATION I2GDIIC

ATEX CERTIFICATION 04.01 EX.02-X

q3
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image83.jpeg
@D® FILTER HOUSING

PART NUMBER
MODEL

TVPE

CARTRIDGE NO. x HEIGHT (inches)
CATEGORY 2014/68/EU

VOLUME LITRES (V)
PRESSURE(PS) min-max bar

TEST PRESSURE(PT) bar
DESIGN TEMPERATURE (TS) min-max 20+ 150°C
FLUID GROUP (2014/68EV) 2
VESSEL MATERIAL 316L/1.4404
YEAR OF MANUFACTURE

VESSEL NUMBER

ATEX CLASSIFICATION n2eplic
ATEX CERTIFICATION 04.01 EX.02X
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TECHNICAL DATA

FILTER HOUSING NAME KMC
CARTRIDGES NUMBER 01
CARTRIDGE SOCKET 226 CODE 7

CERTIFICATION 2014/68/EU (*)

ART 4.3 (no CE mark)
| CAT -only for KMC013 & KMCO014-

DESIGN PRESSURE(PS)

-1+ 10 bar

DESIGN TEMPERATURE(TS) -20 = 150°C
TEST PRESSURE (PT) 14.5 bar
VESSEL MATERIAL AISI 316L W.N. 1.4404

INTERNAL FINISHING

mechanical polishing

INTERNAL ROUGHNESS

Ra=<0.8 micron
-guaranteed only on downstream-

EXTERNAL FINISHING

mechanical polishing
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image88.png
DATA LABEL EXAMPLE

@D®  FILTER HOUSING

PART NUMBER

MODEL

TYPE

CARTRIDGE NO. x HIGH (inch)

CATEGORY CE 2014/68/EU

VOLUME LITRES

PRESSURE(PS) min-max bar

TEST PRESSURE(PT) bar 115

DESIGN TEMPERATURE (TS) min-max -20 +150°C
FLUID GROUP  (Art.13 - 2014/68/EU) 2 - NOT DANG.
VESSEL MATERIAL 316L / 1.4404
YEAR OF MANUFACTURE

VESSEL NUMBER

C € xxxX
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FASTENING SYSTEMS

V] VEE BAND
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image90.png
TECHNICAL DATA

VESSEL RANGE AR

DESIGN CODE EN-13445

FLUID GROUP 2 (NOT DANGEROUS)
PHISICAL STATE GAS

DESIGN PRESSURE (PS) min max 1+ 5 bar

DESIGN TEMPERATURE (TS) max 150°C

TEST PRESSURE (PT) 11.5 bar
CARTRIDGES SOCKET CODE 7

VESSEL MATERIAL 316L / 1.4404

SEALS MATERIAL SILICONE FDA APPROVED
INTERNAL FINISHING UPSTREAM PICKLED

INTERNAL FINISHING DOWNSTREAM
INTERNAL ROUGHNESS DOWNSTREAM
EXTERNAL FINISHING

MECHANICAL POLISHING
RA<0.8 MICRON
SHOT BLASTED

VENT CONNECTION[G

BSP 1/2" FEMALE / CLAMP 1.5"

DRAIN CONNECTION/H]

BSP 1/2" FEMALE / CLAMP 1.5"
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ADVANCED

POS. 1 and 2 ARE ADDED TO BASIC





image94.jpeg
@DP® FILTER HOUSING

PART NUMBER
MODEL

TYPE

CARTRIDGE NO. x HIGH (inch)

CATEGORY 2014/68/EU

VOLUME LITRES (V)

PRESSURE(PS) min-max at TS=-20-40°C bar
PRESSURE(PS) min-max at TS=150°C bar
TEST PRESSURE(PT) bar

DESIGN TEMPERATURE (TS) min-max -20+150°C

FLUID GROUP (At 13 - 2014/68/EU) 1AND 2

VESSEL MATERIAL 316L 7 1.4404
YEAR OF MANUFACTURE

VESSEL NUMBER

ATEX CLASSIFICATION 112GDIIC

ATEX CERTIFICATION 04.01 EX.02X

* THE INDICATED PRESSURES ARE FOR NOT
DANGEROUS LIQUIDS (GROUP 2). FOR THE USE
WITH OTHER FLUIDS SEE THE USER MANUAL.

C€
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TECHNICAL DATA

FILTER HOUSING NAME | VSN

CARTRIDGE SOCKET | 226- COD7

FLUID PHISICAL STATE | GAS

ATEX REGULATION GROUP2 CAT2 GAS&DUST
| FLUID GRIIIC zone 1 & 21

VESSEL MATERIAL aisi 3161/ w.n. 1.4404

INTERNAL FINISHING mechanical polishing

EXTERNAL FINISHING mechanical polishing
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@D®  FILTER HOUSING A

PART NUMBER
MODEL Q"

TYPE

CARTRIDGE NO. x HIGH (inch) N
CATEGORY 2014/68/EU
VOLUME LITRES (V)
PRESSURE(PS) min-max at Ts
PRESSURE(PS) min-max at TS=

20/40°C bar  -1+10 A\
50°C bar A4 A

TEST PRESSURE(PT) bar 20
DESIGN TEMPERATURE (TS) min-max 20+ 150°C
FLUID GROUP (2014/68/EU) 2
VESSEL MATERIAL 316L/1.4404
YEAR OF MANUFACTURE

VESSEL NUMBER

ATEX CLASSIFICATION n26plic
ATEX CERTIFICATION 04,01 EX.02-X

\ SEE USER MANUAL FOR MAX WORKING
PRESSURE WITH NOT DANGEROUS
GAS IN ACCORDANCE WITH 2014/68/EU

CExxxx &
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@D®  FILTER HOUSING

PART NUMBER

MODEL Q"
TYPE

CARTRIDGE NO. x HIGH (inch)
CATEGORY 2014/68/EU
'VOLUME LITRES (V)
PRESSURE(PS) min-max at T¢

20/40°C bar  -1+10 A\

PRESSURE(PS) min-max at TS=150°C bar A+4 A
TEST PRESSURE(PT) bar 20
DESIGN TEMPERATURE (TS) min-max -20 + 150°C
FLUID GROUP (2014/68/EU) 2
VESSEL MATERIAL 316L/ 14404
YEAR OF MANUFACTURE

VESSEL NUMBER

ATEX CLASSIFICATION l26DIc
ATEX CERTIFICATION 04.01 EX.02-X

A\ SEE USER MANUAL FOR MAX WORKING
PRESSURE WITH NOT DANGEROUS
GAS IN ACCORDANCE WITH 2014/68/EU

CExxxx &
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@D®  FILTER HOUSING

PART NUMBER

MODEL

TYPE

CARTRIDGE NO. x HIGH (inch)

CATEGORY 2014/63EU

VOLUME LITRES (V)

PRESSURE(PS) min-max at TS=20/ 40°C bar  -1+10 /A

PRESSURE(PS) min-max at TS=150°C bar A4 A

TEST PRESSURE(PT) bar 20

DESIGN TEMPERATURE (TS) min-max 20+ 150°C

FLUID GROUP (2014/68/EU) 2

VESSEL MATERIAL 316L/1.4404

YEAR OF MANUFACTURE

VESSEL NUMBER

ATEX CLASSIFICATION 126D lIc

ATEX CERTIFICATION 04,01 EX.02-X
£\ SEE USER MANUAL FOR MAX WORKING

PRESSURE WITH NOT DANGEROUS
GAS IN ACCORDANCE WITH 2014/68/EU

CExxxx &
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